<?xml version="1.0"?>
<!-- This file was automatically generated from C sources - DO NOT EDIT!
To affect the contents of this file, edit the original C definitions,
and/or use gtk-doc annotations.  -->
<repository xmlns="http://www.gtk.org/introspection/core/1.0" xmlns:c="http://www.gtk.org/introspection/c/1.0" xmlns:glib="http://www.gtk.org/introspection/glib/1.0" version="1.2">
  <include name="Gst" version="1.0"/>
  <package name="gstreamer-mpegts-1.0"/>
  <c:include name="gst/mpegts/mpegts.h"/>
  <namespace name="GstMpegts" version="1.0" shared-library="libgstmpegts-1.0.so.0" c:identifier-prefixes="GstMpegts" c:symbol-prefixes="gst_mpegts,gst">
    <enumeration name="ATSCDescriptorType" c:type="GstMpegtsATSCDescriptorType">
      <doc xml:space="preserve">These values correspond to the registered descriptor type from
the various ATSC specifications.

Consult the relevant specifications for more details.</doc>
      
      <member name="stuffing" value="128" c:identifier="GST_MTS_DESC_ATSC_STUFFING">
      </member>
      <member name="ac3" value="131" c:identifier="GST_MTS_DESC_ATSC_AC3">
      </member>
      <member name="caption_service" value="134" c:identifier="GST_MTS_DESC_ATSC_CAPTION_SERVICE">
      </member>
      <member name="content_advisory" value="135" c:identifier="GST_MTS_DESC_ATSC_CONTENT_ADVISORY">
      </member>
      <member name="extended_channel_name" value="160" c:identifier="GST_MTS_DESC_ATSC_EXTENDED_CHANNEL_NAME">
      </member>
      <member name="service_location" value="161" c:identifier="GST_MTS_DESC_ATSC_SERVICE_LOCATION">
      </member>
      <member name="time_shifted_service" value="162" c:identifier="GST_MTS_DESC_ATSC_TIME_SHIFTED_SERVICE">
      </member>
      <member name="component_name" value="163" c:identifier="GST_MTS_DESC_ATSC_COMPONENT_NAME">
      </member>
      <member name="dcc_departing_request" value="168" c:identifier="GST_MTS_DESC_ATSC_DCC_DEPARTING_REQUEST">
      </member>
      <member name="dcc_arriving_request" value="169" c:identifier="GST_MTS_DESC_ATSC_DCC_ARRIVING_REQUEST">
      </member>
      <member name="redistribution_control" value="170" c:identifier="GST_MTS_DESC_ATSC_REDISTRIBUTION_CONTROL">
      </member>
      <member name="genre" value="171" c:identifier="GST_MTS_DESC_ATSC_GENRE">
      </member>
      <member name="private_information" value="173" c:identifier="GST_MTS_DESC_ATSC_PRIVATE_INFORMATION">
      </member>
      <member name="eac3" value="204" c:identifier="GST_MTS_DESC_ATSC_EAC3">
      </member>
      <member name="enhanced_signaling" value="178" c:identifier="GST_MTS_DESC_ATSC_ENHANCED_SIGNALING">
      </member>
      <member name="data_service" value="164" c:identifier="GST_MTS_DESC_ATSC_DATA_SERVICE">
      </member>
      <member name="pid_count" value="165" c:identifier="GST_MTS_DESC_ATSC_PID_COUNT">
      </member>
      <member name="download_descriptor" value="166" c:identifier="GST_MTS_DESC_ATSC_DOWNLOAD_DESCRIPTOR">
      </member>
      <member name="multiprotocol_encapsulation" value="167" c:identifier="GST_MTS_DESC_ATSC_MULTIPROTOCOL_ENCAPSULATION">
      </member>
      <member name="module_link" value="180" c:identifier="GST_MTS_DESC_ATSC_MODULE_LINK">
      </member>
      <member name="crc32" value="181" c:identifier="GST_MTS_DESC_ATSC_CRC32">
      </member>
      <member name="group_link" value="184" c:identifier="GST_MTS_DESC_ATSC_GROUP_LINK">
      </member>
    </enumeration>
    <record name="AtscEIT" c:type="GstMpegtsAtscEIT" glib:type-name="GstMpegtsAtscEIT" glib:get-type="gst_mpegts_atsc_eit_get_type" c:symbol-prefix="atsc_eit">
      <doc xml:space="preserve">Event Information Table (ATSC)</doc>
      
      <field name="source_id" writable="1">
        <doc xml:space="preserve">The source id</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="protocol_version" writable="1">
        <doc xml:space="preserve">The protocol version</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="events" writable="1">
        <doc xml:space="preserve">Events</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="AtscEITEvent"/>
        </array>
      </field>
    </record>
    <record name="AtscEITEvent" c:type="GstMpegtsAtscEITEvent" glib:type-name="GstMpegtsAtscEITEvent" glib:get-type="gst_mpegts_atsc_eit_event_get_type" c:symbol-prefix="atsc_eit_event">
      <doc xml:space="preserve">An ATSC EIT Event</doc>
      
      <field name="event_id" writable="1">
        <doc xml:space="preserve">The event id</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="start_time" writable="1">
        <doc xml:space="preserve">The start time</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="etm_location" writable="1">
        <doc xml:space="preserve">The etm location</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="length_in_seconds" writable="1">
        <doc xml:space="preserve">The length in seconds</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="titles" writable="1">
        <doc xml:space="preserve">the titles</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="AtscMultString"/>
        </array>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">descriptors</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
    </record>
    <record name="AtscETT" c:type="GstMpegtsAtscETT" glib:type-name="GstMpegtsAtscETT" glib:get-type="gst_mpegts_atsc_ett_get_type" c:symbol-prefix="atsc_ett">
      <doc xml:space="preserve">Extended Text Table (ATSC)</doc>
      
      <field name="ett_table_id_extension" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="protocol_version" writable="1">
        <doc xml:space="preserve">The protocol version</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="etm_id" writable="1">
        <doc xml:space="preserve">The etm id</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="messages" writable="1">
        <doc xml:space="preserve">List of texts</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="AtscMultString"/>
        </array>
      </field>
    </record>
    <record name="AtscMGT" c:type="GstMpegtsAtscMGT" glib:type-name="GstMpegtsAtscMGT" glib:get-type="gst_mpegts_atsc_mgt_get_type" c:symbol-prefix="atsc_mgt">
      <doc xml:space="preserve">Master Guide Table (A65)</doc>
      
      <field name="protocol_version" writable="1">
        <doc xml:space="preserve">The protocol version</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="tables_defined" writable="1">
        <doc xml:space="preserve">The numbers of subtables</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="tables" writable="1">
        <doc xml:space="preserve">the tables</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="AtscMGTTable"/>
        </array>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">descriptors</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_atsc_mgt_new">
        
        <return-value transfer-ownership="full">
          <type name="AtscMGT" c:type="GstMpegtsAtscMGT*"/>
        </return-value>
      </constructor>
    </record>
    <record name="AtscMGTTable" c:type="GstMpegtsAtscMGTTable" glib:type-name="GstMpegtsAtscMGTTable" glib:get-type="gst_mpegts_atsc_mgt_table_get_type" c:symbol-prefix="atsc_mgt_table">
      <doc xml:space="preserve">Source from a @GstMpegtsAtscMGT</doc>
      
      <field name="table_type" writable="1">
        <doc xml:space="preserve">#GstMpegtsAtscMGTTableType</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="pid" writable="1">
        <doc xml:space="preserve">The packet ID</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="version_number" writable="1">
        <doc xml:space="preserve">The version number</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="number_bytes" writable="1">
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">descriptors</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
    </record>
    <enumeration name="AtscMGTTableType" c:type="GstMpegtsAtscMGTTableType">
      
      <member name="eit0" value="256" c:identifier="GST_MPEGTS_ATSC_MGT_TABLE_TYPE_EIT0">
      </member>
      <member name="eit127" value="383" c:identifier="GST_MPEGTS_ATSC_MGT_TABLE_TYPE_EIT127">
      </member>
      <member name="ett0" value="512" c:identifier="GST_MPEGTS_ATSC_MGT_TABLE_TYPE_ETT0">
      </member>
      <member name="ett127" value="639" c:identifier="GST_MPEGTS_ATSC_MGT_TABLE_TYPE_ETT127">
      </member>
    </enumeration>
    <record name="AtscMultString" c:type="GstMpegtsAtscMultString" glib:type-name="GstMpegtsAtscMultString" glib:get-type="gst_mpegts_atsc_mult_string_get_type" c:symbol-prefix="atsc_mult_string">
      
      <field name="iso_639_langcode" writable="1">
        <doc xml:space="preserve">The ISO639 language code</doc>
        <array zero-terminated="0" fixed-size="4">
          <type name="gchar" c:type="gchar"/>
        </array>
      </field>
      <field name="segments" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="AtscStringSegment"/>
        </array>
      </field>
    </record>
    <record name="AtscRRT" c:type="GstMpegtsAtscRRT" version="1.18" glib:type-name="GstMpegtsAtscRRT" glib:get-type="gst_mpegts_atsc_rrt_get_type" c:symbol-prefix="atsc_rrt">
      <doc xml:space="preserve">Region Rating Table (A65)</doc>
      
      <field name="protocol_version" writable="1">
        <doc xml:space="preserve">The protocol version</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="names" writable="1">
        <doc xml:space="preserve">the names</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="AtscMultString"/>
        </array>
      </field>
      <field name="dimensions_defined" writable="1">
        <doc xml:space="preserve">the number of dimensions defined for this rating table</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="dimensions" writable="1">
        <doc xml:space="preserve">A set of dimensions</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="AtscRRTDimension"/>
        </array>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">descriptors</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="gpointer" c:type="gpointer"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_atsc_rrt_new">
        
        <return-value transfer-ownership="full">
          <type name="AtscRRT" c:type="GstMpegtsAtscRRT*"/>
        </return-value>
      </constructor>
    </record>
    <record name="AtscRRTDimension" c:type="GstMpegtsAtscRRTDimension" glib:type-name="GstMpegtsAtscRRTDimension" glib:get-type="gst_mpegts_atsc_rrt_dimension_get_type" c:symbol-prefix="atsc_rrt_dimension">
      
      <field name="names" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="gpointer" c:type="gpointer"/>
        </array>
      </field>
      <field name="graduated_scale" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="values_defined" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="values" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="gpointer" c:type="gpointer"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_atsc_rrt_dimension_new">
        
        <return-value transfer-ownership="full">
          <type name="AtscRRTDimension" c:type="GstMpegtsAtscRRTDimension*"/>
        </return-value>
      </constructor>
    </record>
    <record name="AtscRRTDimensionValue" c:type="GstMpegtsAtscRRTDimensionValue" version="1.18" glib:type-name="GstMpegtsAtscRRTDimensionValue" glib:get-type="gst_mpegts_atsc_rrt_dimension_value_get_type" c:symbol-prefix="atsc_rrt_dimension_value">
      
      <field name="abbrev_ratings" writable="1">
        <doc xml:space="preserve">the abbreviated ratings</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="AtscMultString"/>
        </array>
      </field>
      <field name="ratings" writable="1">
        <doc xml:space="preserve">the ratings</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="AtscMultString"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_atsc_rrt_dimension_value_new">
        
        <return-value transfer-ownership="full">
          <type name="AtscRRTDimensionValue" c:type="GstMpegtsAtscRRTDimensionValue*"/>
        </return-value>
      </constructor>
    </record>
    <record name="AtscSTT" c:type="GstMpegtsAtscSTT" glib:type-name="GstMpegtsAtscSTT" glib:get-type="gst_mpegts_atsc_stt_get_type" c:symbol-prefix="atsc_stt">
      <doc xml:space="preserve">System Time Table (A65)</doc>
      
      <field name="protocol_version" writable="1">
        <doc xml:space="preserve">The protocol version</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="system_time" writable="1">
        <doc xml:space="preserve">The system time</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="gps_utc_offset" writable="1">
        <doc xml:space="preserve">The GPS to UTC offset</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="ds_status" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="ds_dayofmonth" writable="1">
        <doc xml:space="preserve">The day of month</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="ds_hour" writable="1">
        <doc xml:space="preserve">The hour</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">descriptors</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
      <field name="utc_datetime" writable="1">
        <doc xml:space="preserve">The UTC date and time</doc>
        <type name="Gst.DateTime" c:type="GstDateTime*"/>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_atsc_stt_new">
        
        <return-value transfer-ownership="full">
          <type name="AtscSTT" c:type="GstMpegtsAtscSTT*"/>
        </return-value>
      </constructor>
      <method name="get_datetime_utc" c:identifier="gst_mpegts_atsc_stt_get_datetime_utc">
        
        <return-value transfer-ownership="full">
          <type name="Gst.DateTime" c:type="GstDateTime*"/>
        </return-value>
        <parameters>
          <instance-parameter name="stt" transfer-ownership="none">
            <type name="AtscSTT" c:type="GstMpegtsAtscSTT*"/>
          </instance-parameter>
        </parameters>
      </method>
    </record>
    <record name="AtscStringSegment" c:type="GstMpegtsAtscStringSegment" glib:type-name="GstMpegtsAtscStringSegment" glib:get-type="gst_mpegts_atsc_string_segment_get_type" c:symbol-prefix="atsc_string_segment">
      <doc xml:space="preserve">A string segment</doc>
      
      <field name="compression_type" writable="1">
        <doc xml:space="preserve">The compression type</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="mode" writable="1">
        <doc xml:space="preserve">The mode</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="compressed_data_size" writable="1">
        <doc xml:space="preserve">The size of compressed data</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="compressed_data" writable="1">
        <doc xml:space="preserve">The compressed data</doc>
        <type name="guint8" c:type="guint8*"/>
      </field>
      <field name="cached_string" writable="1">
        <type name="utf8" c:type="gchar*"/>
      </field>
      <method name="get_string" c:identifier="gst_mpegts_atsc_string_segment_get_string">
        
        <return-value transfer-ownership="none">
          <type name="utf8" c:type="const gchar*"/>
        </return-value>
        <parameters>
          <instance-parameter name="seg" transfer-ownership="none">
            <type name="AtscStringSegment" c:type="GstMpegtsAtscStringSegment*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="set_string" c:identifier="gst_mpegts_atsc_string_segment_set_string">
        
        <return-value transfer-ownership="none">
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="seg" transfer-ownership="none">
            <type name="AtscStringSegment" c:type="GstMpegtsAtscStringSegment*"/>
          </instance-parameter>
          <parameter name="string" transfer-ownership="none">
            <type name="utf8" c:type="gchar*"/>
          </parameter>
          <parameter name="compression_type" transfer-ownership="none">
            <type name="guint8" c:type="guint8"/>
          </parameter>
          <parameter name="mode" transfer-ownership="none">
            <type name="guint8" c:type="guint8"/>
          </parameter>
        </parameters>
      </method>
    </record>
    <record name="AtscVCT" c:type="GstMpegtsAtscVCT" glib:type-name="GstMpegtsAtscVCT" glib:get-type="gst_mpegts_atsc_vct_get_type" c:symbol-prefix="atsc_vct">
      <doc xml:space="preserve">Represents both:
  Terrestrial Virtual Channel Table (A65)
  Cable Virtual Channel Table (A65)</doc>
      
      <field name="transport_stream_id" writable="1">
        <doc xml:space="preserve">The transport stream</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="protocol_version" writable="1">
        <doc xml:space="preserve">The protocol version</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="sources" writable="1">
        <doc xml:space="preserve">sources</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="AtscVCTSource"/>
        </array>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">descriptors</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
    </record>
    <record name="AtscVCTSource" c:type="GstMpegtsAtscVCTSource" glib:type-name="GstMpegtsAtscVCTSource" glib:get-type="gst_mpegts_atsc_vct_source_get_type" c:symbol-prefix="atsc_vct_source">
      <doc xml:space="preserve">Source from a @GstMpegtsAtscVCT, can be used both for TVCT and CVCT tables</doc>
      
      <field name="short_name" writable="1">
        <doc xml:space="preserve">The short name of a source</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="major_channel_number" writable="1">
        <doc xml:space="preserve">The major channel number</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="minor_channel_number" writable="1">
        <doc xml:space="preserve">The minor channel number</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="modulation_mode" writable="1">
        <doc xml:space="preserve">The modulation mode</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="carrier_frequency" writable="1">
        <doc xml:space="preserve">The carrier frequency</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="channel_TSID" writable="1">
        <doc xml:space="preserve">The transport stream ID</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="program_number" writable="1">
        <doc xml:space="preserve">The program number (see #GstMpegtsPatProgram)</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="ETM_location" writable="1">
        <doc xml:space="preserve">The ETM location</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="access_controlled" writable="1">
        <doc xml:space="preserve">is access controlled</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="hidden" writable="1">
        <doc xml:space="preserve">is hidden</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="path_select" writable="1">
        <doc xml:space="preserve">is path select, CVCT only</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="out_of_band" writable="1">
        <doc xml:space="preserve">is out of band, CVCT only</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="hide_guide" writable="1">
        <doc xml:space="preserve">is hide guide</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="service_type" writable="1">
        <doc xml:space="preserve">The service type</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="source_id" writable="1">
        <doc xml:space="preserve">The source id</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">an array of #GstMpegtsDescriptor</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
    </record>
    <record name="BAT" c:type="GstMpegtsBAT" glib:type-name="GstMpegtsBAT" glib:get-type="gst_mpegts_bat_get_type" c:symbol-prefix="bat">
      <doc xml:space="preserve">DVB Bouquet Association Table (EN 300 468)</doc>
      
      <field name="descriptors" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
      <field name="streams" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="BATStream"/>
        </array>
      </field>
    </record>
    <record name="BATStream" c:type="GstMpegtsBATStream" glib:type-name="GstMpegtsBATStream" glib:get-type="gst_mpegts_bat_stream_get_type" c:symbol-prefix="bat_stream">
      
      <field name="transport_stream_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="original_network_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="descriptors" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="gpointer" c:type="gpointer"/>
        </array>
      </field>
    </record>
    <record name="CableDeliverySystemDescriptor" c:type="GstMpegtsCableDeliverySystemDescriptor" glib:type-name="GstMpegtsCableDeliverySystemDescriptor" glib:get-type="gst_mpegts_dvb_cable_delivery_system_descriptor_get_type" c:symbol-prefix="dvb_cable_delivery_system_descriptor">
      <doc xml:space="preserve">Cable Delivery System Descriptor (EN 300 468 v.1.13.1)</doc>
      
      <field name="frequency" writable="1">
        <doc xml:space="preserve">the frequency in Hz (Hertz)</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="outer_fec" writable="1">
        <doc xml:space="preserve">the outer FEC scheme used</doc>
        <type name="CableOuterFECScheme" c:type="GstMpegtsCableOuterFECScheme"/>
      </field>
      <field name="modulation" writable="1">
        <doc xml:space="preserve">Modulation scheme used</doc>
        <type name="ModulationType" c:type="GstMpegtsModulationType"/>
      </field>
      <field name="symbol_rate" writable="1">
        <doc xml:space="preserve">Symbol rate (in symbols per second)</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="fec_inner" writable="1">
        <doc xml:space="preserve">inner FEC scheme used</doc>
        <type name="DVBCodeRate" c:type="GstMpegtsDVBCodeRate"/>
      </field>
      <method name="free" c:identifier="gst_mpegts_dvb_cable_delivery_system_descriptor_free">
        
        <return-value transfer-ownership="none">
          <type name="none" c:type="void"/>
        </return-value>
        <parameters>
          <instance-parameter name="source" transfer-ownership="none">
            <type name="CableDeliverySystemDescriptor" c:type="GstMpegtsCableDeliverySystemDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
    </record>
    <enumeration name="CableOuterFECScheme" c:type="GstMpegtsCableOuterFECScheme">
      
      <member name="undefined" value="0" c:identifier="GST_MPEGTS_CABLE_OUTER_FEC_UNDEFINED">
      </member>
      <member name="none" value="1" c:identifier="GST_MPEGTS_CABLE_OUTER_FEC_NONE">
      </member>
      <member name="rs_204_188" value="2" c:identifier="GST_MPEGTS_CABLE_OUTER_FEC_RS_204_188">
      </member>
    </enumeration>
    <record name="ComponentDescriptor" c:type="GstMpegtsComponentDescriptor" glib:type-name="GstMpegtsComponentDescriptor" glib:get-type="gst_mpegts_component_descriptor_get_type" c:symbol-prefix="component_descriptor">
      
      <field name="stream_content" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="component_type" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="component_tag" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="language_code" writable="1">
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="text" writable="1">
        <type name="utf8" c:type="gchar*"/>
      </field>
    </record>
    <enumeration name="ComponentStreamContent" c:type="GstMpegtsComponentStreamContent">
      
      <member name="mpeg2_video" value="1" c:identifier="GST_MPEGTS_STREAM_CONTENT_MPEG2_VIDEO">
      </member>
      <member name="mpeg1_layer2_audio" value="2" c:identifier="GST_MPEGTS_STREAM_CONTENT_MPEG1_LAYER2_AUDIO">
      </member>
      <member name="teletext_or_subtitle" value="3" c:identifier="GST_MPEGTS_STREAM_CONTENT_TELETEXT_OR_SUBTITLE">
      </member>
      <member name="ac_3" value="4" c:identifier="GST_MPEGTS_STREAM_CONTENT_AC_3">
      </member>
      <member name="avc" value="5" c:identifier="GST_MPEGTS_STREAM_CONTENT_AVC">
      </member>
      <member name="aac" value="6" c:identifier="GST_MPEGTS_STREAM_CONTENT_AAC">
      </member>
      <member name="dts" value="7" c:identifier="GST_MPEGTS_STREAM_CONTENT_DTS">
      </member>
      <member name="srm_cpcm" value="8" c:identifier="GST_MPEGTS_STREAM_CONTENT_SRM_CPCM">
      </member>
    </enumeration>
    <record name="Content" c:type="GstMpegtsContent" glib:type-name="GstMpegtsContent" glib:get-type="gst_mpegts_content_get_type" c:symbol-prefix="content">
      
      <field name="content_nibble_1" writable="1">
        <type name="ContentNibbleHi" c:type="GstMpegtsContentNibbleHi"/>
      </field>
      <field name="content_nibble_2" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="user_byte" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
    </record>
    <enumeration name="ContentNibbleHi" c:type="GstMpegtsContentNibbleHi">
      
      <member name="movie_drama" value="1" c:identifier="GST_MPEGTS_CONTENT_MOVIE_DRAMA">
      </member>
      <member name="news_current_affairs" value="2" c:identifier="GST_MPEGTS_CONTENT_NEWS_CURRENT_AFFAIRS">
      </member>
      <member name="show_game_show" value="3" c:identifier="GST_MPEGTS_CONTENT_SHOW_GAME_SHOW">
      </member>
      <member name="sports" value="4" c:identifier="GST_MPEGTS_CONTENT_SPORTS">
      </member>
      <member name="children_youth_program" value="5" c:identifier="GST_MPEGTS_CONTENT_CHILDREN_YOUTH_PROGRAM">
      </member>
      <member name="music_ballet_dance" value="6" c:identifier="GST_MPEGTS_CONTENT_MUSIC_BALLET_DANCE">
      </member>
      <member name="arts_culture" value="7" c:identifier="GST_MPEGTS_CONTENT_ARTS_CULTURE">
      </member>
      <member name="social_political_economics" value="8" c:identifier="GST_MPEGTS_CONTENT_SOCIAL_POLITICAL_ECONOMICS">
      </member>
      <member name="education_science_factual" value="9" c:identifier="GST_MPEGTS_CONTENT_EDUCATION_SCIENCE_FACTUAL">
      </member>
      <member name="leisure_hobbies" value="10" c:identifier="GST_MPEGTS_CONTENT_LEISURE_HOBBIES">
      </member>
      <member name="special_characteristics" value="11" c:identifier="GST_MPEGTS_CONTENT_SPECIAL_CHARACTERISTICS">
      </member>
    </enumeration>
    <enumeration name="DVBCodeRate" c:type="GstMpegtsDVBCodeRate">
      
      <member name="none" value="0" c:identifier="GST_MPEGTS_FEC_NONE">
      </member>
      <member name="1_2" value="1" c:identifier="GST_MPEGTS_FEC_1_2">
      </member>
      <member name="2_3" value="2" c:identifier="GST_MPEGTS_FEC_2_3">
      </member>
      <member name="3_4" value="3" c:identifier="GST_MPEGTS_FEC_3_4">
      </member>
      <member name="4_5" value="4" c:identifier="GST_MPEGTS_FEC_4_5">
      </member>
      <member name="5_6" value="5" c:identifier="GST_MPEGTS_FEC_5_6">
      </member>
      <member name="6_7" value="6" c:identifier="GST_MPEGTS_FEC_6_7">
      </member>
      <member name="7_8" value="7" c:identifier="GST_MPEGTS_FEC_7_8">
      </member>
      <member name="8_9" value="8" c:identifier="GST_MPEGTS_FEC_8_9">
      </member>
      <member name="auto" value="9" c:identifier="GST_MPEGTS_FEC_AUTO">
      </member>
      <member name="3_5" value="10" c:identifier="GST_MPEGTS_FEC_3_5">
      </member>
      <member name="9_10" value="11" c:identifier="GST_MPEGTS_FEC_9_10">
      </member>
      <member name="2_5" value="12" c:identifier="GST_MPEGTS_FEC_2_5">
      </member>
    </enumeration>
    <enumeration name="DVBDescriptorType" c:type="GstMpegtsDVBDescriptorType">
      <doc xml:space="preserve">The type of #GstMpegtsDescriptor

These values correspond to the registered descriptor type from
the various DVB specifications.

Consult the relevant specifications for more details.</doc>
      
      <member name="network_name" value="64" c:identifier="GST_MTS_DESC_DVB_NETWORK_NAME">
      </member>
      <member name="service_list" value="65" c:identifier="GST_MTS_DESC_DVB_SERVICE_LIST">
      </member>
      <member name="stuffing" value="66" c:identifier="GST_MTS_DESC_DVB_STUFFING">
      </member>
      <member name="satellite_delivery_system" value="67" c:identifier="GST_MTS_DESC_DVB_SATELLITE_DELIVERY_SYSTEM">
      </member>
      <member name="cable_delivery_system" value="68" c:identifier="GST_MTS_DESC_DVB_CABLE_DELIVERY_SYSTEM">
      </member>
      <member name="vbi_data" value="69" c:identifier="GST_MTS_DESC_DVB_VBI_DATA">
      </member>
      <member name="vbi_teletext" value="70" c:identifier="GST_MTS_DESC_DVB_VBI_TELETEXT">
      </member>
      <member name="bouquet_name" value="71" c:identifier="GST_MTS_DESC_DVB_BOUQUET_NAME">
      </member>
      <member name="service" value="72" c:identifier="GST_MTS_DESC_DVB_SERVICE">
      </member>
      <member name="country_availability" value="73" c:identifier="GST_MTS_DESC_DVB_COUNTRY_AVAILABILITY">
      </member>
      <member name="linkage" value="74" c:identifier="GST_MTS_DESC_DVB_LINKAGE">
      </member>
      <member name="nvod_reference" value="75" c:identifier="GST_MTS_DESC_DVB_NVOD_REFERENCE">
      </member>
      <member name="time_shifted_service" value="76" c:identifier="GST_MTS_DESC_DVB_TIME_SHIFTED_SERVICE">
      </member>
      <member name="short_event" value="77" c:identifier="GST_MTS_DESC_DVB_SHORT_EVENT">
      </member>
      <member name="extended_event" value="78" c:identifier="GST_MTS_DESC_DVB_EXTENDED_EVENT">
      </member>
      <member name="time_shifted_event" value="79" c:identifier="GST_MTS_DESC_DVB_TIME_SHIFTED_EVENT">
      </member>
      <member name="component" value="80" c:identifier="GST_MTS_DESC_DVB_COMPONENT">
      </member>
      <member name="mosaic" value="81" c:identifier="GST_MTS_DESC_DVB_MOSAIC">
      </member>
      <member name="stream_identifier" value="82" c:identifier="GST_MTS_DESC_DVB_STREAM_IDENTIFIER">
      </member>
      <member name="ca_identifier" value="83" c:identifier="GST_MTS_DESC_DVB_CA_IDENTIFIER">
      </member>
      <member name="content" value="84" c:identifier="GST_MTS_DESC_DVB_CONTENT">
      </member>
      <member name="parental_rating" value="85" c:identifier="GST_MTS_DESC_DVB_PARENTAL_RATING">
      </member>
      <member name="teletext" value="86" c:identifier="GST_MTS_DESC_DVB_TELETEXT">
      </member>
      <member name="telephone" value="87" c:identifier="GST_MTS_DESC_DVB_TELEPHONE">
      </member>
      <member name="local_time_offset" value="88" c:identifier="GST_MTS_DESC_DVB_LOCAL_TIME_OFFSET">
      </member>
      <member name="subtitling" value="89" c:identifier="GST_MTS_DESC_DVB_SUBTITLING">
      </member>
      <member name="terrestrial_delivery_system" value="90" c:identifier="GST_MTS_DESC_DVB_TERRESTRIAL_DELIVERY_SYSTEM">
      </member>
      <member name="multilingual_network_name" value="91" c:identifier="GST_MTS_DESC_DVB_MULTILINGUAL_NETWORK_NAME">
      </member>
      <member name="multilingual_bouquet_name" value="92" c:identifier="GST_MTS_DESC_DVB_MULTILINGUAL_BOUQUET_NAME">
      </member>
      <member name="multilingual_service_name" value="93" c:identifier="GST_MTS_DESC_DVB_MULTILINGUAL_SERVICE_NAME">
      </member>
      <member name="multilingual_component" value="94" c:identifier="GST_MTS_DESC_DVB_MULTILINGUAL_COMPONENT">
      </member>
      <member name="private_data_specifier" value="95" c:identifier="GST_MTS_DESC_DVB_PRIVATE_DATA_SPECIFIER">
      </member>
      <member name="service_move" value="96" c:identifier="GST_MTS_DESC_DVB_SERVICE_MOVE">
      </member>
      <member name="short_smoothing_buffer" value="97" c:identifier="GST_MTS_DESC_DVB_SHORT_SMOOTHING_BUFFER">
      </member>
      <member name="frequency_list" value="98" c:identifier="GST_MTS_DESC_DVB_FREQUENCY_LIST">
      </member>
      <member name="partial_transport_stream" value="99" c:identifier="GST_MTS_DESC_DVB_PARTIAL_TRANSPORT_STREAM">
      </member>
      <member name="data_broadcast" value="100" c:identifier="GST_MTS_DESC_DVB_DATA_BROADCAST">
      </member>
      <member name="scrambling" value="101" c:identifier="GST_MTS_DESC_DVB_SCRAMBLING">
      </member>
      <member name="data_broadcast_id" value="102" c:identifier="GST_MTS_DESC_DVB_DATA_BROADCAST_ID">
      </member>
      <member name="transport_stream" value="103" c:identifier="GST_MTS_DESC_DVB_TRANSPORT_STREAM">
      </member>
      <member name="dsng" value="104" c:identifier="GST_MTS_DESC_DVB_DSNG">
      </member>
      <member name="pdc" value="105" c:identifier="GST_MTS_DESC_DVB_PDC">
      </member>
      <member name="ac3" value="106" c:identifier="GST_MTS_DESC_DVB_AC3">
      </member>
      <member name="ancillary_data" value="107" c:identifier="GST_MTS_DESC_DVB_ANCILLARY_DATA">
      </member>
      <member name="cell_list" value="108" c:identifier="GST_MTS_DESC_DVB_CELL_LIST">
      </member>
      <member name="cell_frequency_link" value="109" c:identifier="GST_MTS_DESC_DVB_CELL_FREQUENCY_LINK">
      </member>
      <member name="announcement_support" value="110" c:identifier="GST_MTS_DESC_DVB_ANNOUNCEMENT_SUPPORT">
      </member>
      <member name="application_signalling" value="111" c:identifier="GST_MTS_DESC_DVB_APPLICATION_SIGNALLING">
      </member>
      <member name="adaptation_field_data" value="112" c:identifier="GST_MTS_DESC_DVB_ADAPTATION_FIELD_DATA">
      </member>
      <member name="service_identifier" value="113" c:identifier="GST_MTS_DESC_DVB_SERVICE_IDENTIFIER">
      </member>
      <member name="service_availability" value="114" c:identifier="GST_MTS_DESC_DVB_SERVICE_AVAILABILITY">
      </member>
      <member name="default_authority" value="115" c:identifier="GST_MTS_DESC_DVB_DEFAULT_AUTHORITY">
      </member>
      <member name="related_content" value="116" c:identifier="GST_MTS_DESC_DVB_RELATED_CONTENT">
      </member>
      <member name="tva_id" value="117" c:identifier="GST_MTS_DESC_DVB_TVA_ID">
      </member>
      <member name="content_identifier" value="118" c:identifier="GST_MTS_DESC_DVB_CONTENT_IDENTIFIER">
      </member>
      <member name="timeslice_fec_identifier" value="119" c:identifier="GST_MTS_DESC_DVB_TIMESLICE_FEC_IDENTIFIER">
      </member>
      <member name="ecm_repetition_rate" value="120" c:identifier="GST_MTS_DESC_DVB_ECM_REPETITION_RATE">
      </member>
      <member name="s2_satellite_delivery_system" value="121" c:identifier="GST_MTS_DESC_DVB_S2_SATELLITE_DELIVERY_SYSTEM">
      </member>
      <member name="enhanced_ac3" value="122" c:identifier="GST_MTS_DESC_DVB_ENHANCED_AC3">
      </member>
      <member name="dts" value="123" c:identifier="GST_MTS_DESC_DVB_DTS">
      </member>
      <member name="aac" value="124" c:identifier="GST_MTS_DESC_DVB_AAC">
      </member>
      <member name="xait_location" value="125" c:identifier="GST_MTS_DESC_DVB_XAIT_LOCATION">
      </member>
      <member name="fta_content_management" value="126" c:identifier="GST_MTS_DESC_DVB_FTA_CONTENT_MANAGEMENT">
      </member>
      <member name="extension" value="127" c:identifier="GST_MTS_DESC_DVB_EXTENSION">
      </member>
    </enumeration>
    <enumeration name="DVBExtendedDescriptorType" c:type="GstMpegtsDVBExtendedDescriptorType">
      <doc xml:space="preserve">The type of #GstMpegtsDescriptor

These values correspond to the registered extended descriptor
type from the various DVB specifications.

Consult the relevant specifications for more details.</doc>
      
      <member name="image_icon" value="0" c:identifier="GST_MTS_DESC_EXT_DVB_IMAGE_ICON">
      </member>
      <member name="cpcm_delivery_signalling" value="1" c:identifier="GST_MTS_DESC_EXT_DVB_CPCM_DELIVERY_SIGNALLING">
      </member>
      <member name="cp" value="2" c:identifier="GST_MTS_DESC_EXT_DVB_CP">
      </member>
      <member name="cp_identifier" value="3" c:identifier="GST_MTS_DESC_EXT_DVB_CP_IDENTIFIER">
      </member>
      <member name="t2_delivery_system" value="4" c:identifier="GST_MTS_DESC_EXT_DVB_T2_DELIVERY_SYSTEM">
      </member>
      <member name="sh_delivery_system" value="5" c:identifier="GST_MTS_DESC_EXT_DVB_SH_DELIVERY_SYSTEM">
      </member>
      <member name="supplementary_audio" value="6" c:identifier="GST_MTS_DESC_EXT_DVB_SUPPLEMENTARY_AUDIO">
      </member>
      <member name="network_change_notify" value="7" c:identifier="GST_MTS_DESC_EXT_DVB_NETWORK_CHANGE_NOTIFY">
      </member>
      <member name="message" value="8" c:identifier="GST_MTS_DESC_EXT_DVB_MESSAGE">
      </member>
      <member name="target_region" value="9" c:identifier="GST_MTS_DESC_EXT_DVB_TARGET_REGION">
      </member>
      <member name="target_region_name" value="10" c:identifier="GST_MTS_DESC_EXT_DVB_TARGET_REGION_NAME">
      </member>
      <member name="service_relocated" value="11" c:identifier="GST_MTS_DESC_EXT_DVB_SERVICE_RELOCATED">
      </member>
      <member name="xait_pid" value="12" c:identifier="GST_MTS_DESC_EXT_DVB_XAIT_PID">
      </member>
      <member name="c2_delivery_system" value="13" c:identifier="GST_MTS_DESC_EXT_DVB_C2_DELIVERY_SYSTEM">
      </member>
      <member name="dts_hd_audio_stream" value="14" c:identifier="GST_MTS_DESC_EXT_DVB_DTS_HD_AUDIO_STREAM">
      </member>
      <member name="dts_neutral" value="15" c:identifier="GST_MTS_DESC_EXT_DVB_DTS_NEUTRAL">
      </member>
      <member name="video_depth_range" value="16" c:identifier="GST_MTS_DESC_EXT_DVB_VIDEO_DEPTH_RANGE">
      </member>
      <member name="t2mi" value="17" c:identifier="GST_MTS_DESC_EXT_DVB_T2MI">
      </member>
      <member name="uri_linkage" value="19" c:identifier="GST_MTS_DESC_EXT_DVB_URI_LINKAGE">
      </member>
      <member name="ac4" value="21" c:identifier="GST_MTS_DESC_EXT_DVB_AC4">
      </member>
    </enumeration>
    <record name="DVBLinkageDescriptor" c:type="GstMpegtsDVBLinkageDescriptor" glib:type-name="GstMpegtsDVBLinkageDescriptor" glib:get-type="gst_mpegts_dvb_linkage_descriptor_get_type" c:symbol-prefix="dvb_linkage_descriptor">
      
      <field name="transport_stream_id" writable="1">
        <doc xml:space="preserve">the transport id</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="original_network_id" writable="1">
        <doc xml:space="preserve">the original network id</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="service_id" writable="1">
        <doc xml:space="preserve">the service id</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="linkage_type" writable="1">
        <doc xml:space="preserve">the type which @linkage_data has</doc>
        <type name="DVBLinkageType" c:type="GstMpegtsDVBLinkageType"/>
      </field>
      <field name="linkage_data" readable="0" private="1">
        <type name="gpointer" c:type="gpointer"/>
      </field>
      <field name="private_data_length" writable="1">
        <doc xml:space="preserve">the length for @private_data_bytes</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="private_data_bytes" writable="1">
        <doc xml:space="preserve">additional data bytes</doc>
        <type name="guint8" c:type="guint8*"/>
      </field>
      <method name="free" c:identifier="gst_mpegts_dvb_linkage_descriptor_free">
        
        <return-value transfer-ownership="none">
          <type name="none" c:type="void"/>
        </return-value>
        <parameters>
          <instance-parameter name="source" transfer-ownership="none">
            <type name="DVBLinkageDescriptor" c:type="GstMpegtsDVBLinkageDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_event" c:identifier="gst_mpegts_dvb_linkage_descriptor_get_event">
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsDVBLinkageEvent or %NULL if an error happened</doc>
          <type name="DVBLinkageEvent" c:type="const GstMpegtsDVBLinkageEvent*"/>
        </return-value>
        <parameters>
          <instance-parameter name="desc" transfer-ownership="none">
            <doc xml:space="preserve">the #GstMpegtsDVBLinkageDescriptor</doc>
            <type name="DVBLinkageDescriptor" c:type="const GstMpegtsDVBLinkageDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_extended_event" c:identifier="gst_mpegts_dvb_linkage_descriptor_get_extended_event">
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">an #GstMpegtsDVBLinkageExtendedEvent array or %NULL if an error happened</doc>
          <array name="GLib.PtrArray" c:type="const GPtrArray*">
            <type name="DVBLinkageExtendedEvent"/>
          </array>
        </return-value>
        <parameters>
          <instance-parameter name="desc" transfer-ownership="none">
            <doc xml:space="preserve">the #GstMpegtsDVBLinkageDescriptor</doc>
            <type name="DVBLinkageDescriptor" c:type="const GstMpegtsDVBLinkageDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_mobile_hand_over" c:identifier="gst_mpegts_dvb_linkage_descriptor_get_mobile_hand_over">
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsDVBLinkageMobileHandOver or %NULL if an error happened</doc>
          <type name="DVBLinkageMobileHandOver" c:type="const GstMpegtsDVBLinkageMobileHandOver*"/>
        </return-value>
        <parameters>
          <instance-parameter name="desc" transfer-ownership="none">
            <doc xml:space="preserve">the #GstMpegtsDVBLinkageDescriptor</doc>
            <type name="DVBLinkageDescriptor" c:type="const GstMpegtsDVBLinkageDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
    </record>
    <record name="DVBLinkageEvent" c:type="GstMpegtsDVBLinkageEvent" glib:type-name="GstMpegtsDVBLinkageEvent" glib:get-type="gst_mpegts_dvb_linkage_event_get_type" c:symbol-prefix="dvb_linkage_event">
      
      <field name="target_event_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="target_listed" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="event_simulcast" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
    </record>
    <record name="DVBLinkageExtendedEvent" c:type="GstMpegtsDVBLinkageExtendedEvent" glib:type-name="GstMpegtsDVBLinkageExtendedEvent" glib:get-type="gst_mpegts_dvb_linkage_extended_event_get_type" c:symbol-prefix="dvb_linkage_extended_event">
      
      <field name="target_event_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="target_listed" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="event_simulcast" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="link_type" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="target_id_type" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="original_network_id_flag" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="service_id_flag" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="user_defined_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="target_transport_stream_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="target_original_network_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="target_service_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
    </record>
    <enumeration name="DVBLinkageHandOverType" c:type="GstMpegtsDVBLinkageHandOverType">
      
      <member name="reserved" value="0" c:identifier="GST_MPEGTS_DVB_LINKAGE_HAND_OVER_RESERVED">
      </member>
      <member name="identical" value="1" c:identifier="GST_MPEGTS_DVB_LINKAGE_HAND_OVER_IDENTICAL">
      </member>
      <member name="local_variation" value="2" c:identifier="GST_MPEGTS_DVB_LINKAGE_HAND_OVER_LOCAL_VARIATION">
      </member>
      <member name="associated" value="3" c:identifier="GST_MPEGTS_DVB_LINKAGE_HAND_OVER_ASSOCIATED">
      </member>
    </enumeration>
    <record name="DVBLinkageMobileHandOver" c:type="GstMpegtsDVBLinkageMobileHandOver" glib:type-name="GstMpegtsDVBLinkageMobileHandOver" glib:get-type="gst_mpegts_dvb_linkage_mobile_hand_over_get_type" c:symbol-prefix="dvb_linkage_mobile_hand_over">
      
      <field name="hand_over_type" writable="1">
        <type name="DVBLinkageHandOverType" c:type="GstMpegtsDVBLinkageHandOverType"/>
      </field>
      <field name="origin_type" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="network_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="initial_service_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
    </record>
    <enumeration name="DVBLinkageType" c:type="GstMpegtsDVBLinkageType">
      <doc xml:space="preserve">Linkage Type (EN 300 468 v.1.13.1)</doc>
      
      <member name="reserved_00" value="0" c:identifier="GST_MPEGTS_DVB_LINKAGE_RESERVED_00">
      </member>
      <member name="information" value="1" c:identifier="GST_MPEGTS_DVB_LINKAGE_INFORMATION">
      </member>
      <member name="epg" value="2" c:identifier="GST_MPEGTS_DVB_LINKAGE_EPG">
      </member>
      <member name="ca_replacement" value="3" c:identifier="GST_MPEGTS_DVB_LINKAGE_CA_REPLACEMENT">
      </member>
      <member name="ts_containing_complete_si" value="4" c:identifier="GST_MPEGTS_DVB_LINKAGE_TS_CONTAINING_COMPLETE_SI">
      </member>
      <member name="service_replacement" value="5" c:identifier="GST_MPEGTS_DVB_LINKAGE_SERVICE_REPLACEMENT">
      </member>
      <member name="data_broadcast" value="6" c:identifier="GST_MPEGTS_DVB_LINKAGE_DATA_BROADCAST">
      </member>
      <member name="rcs_map" value="7" c:identifier="GST_MPEGTS_DVB_LINKAGE_RCS_MAP">
      </member>
      <member name="mobile_hand_over" value="8" c:identifier="GST_MPEGTS_DVB_LINKAGE_MOBILE_HAND_OVER">
      </member>
      <member name="system_software_update" value="9" c:identifier="GST_MPEGTS_DVB_LINKAGE_SYSTEM_SOFTWARE_UPDATE">
      </member>
      <member name="ts_containing_ssu" value="10" c:identifier="GST_MPEGTS_DVB_LINKAGE_TS_CONTAINING_SSU">
      </member>
      <member name="ip_mac_notification" value="11" c:identifier="GST_MPEGTS_DVB_LINKAGE_IP_MAC_NOTIFICATION">
      </member>
      <member name="ts_containing_int" value="12" c:identifier="GST_MPEGTS_DVB_LINKAGE_TS_CONTAINING_INT">
      </member>
      <member name="event" value="13" c:identifier="GST_MPEGTS_DVB_LINKAGE_EVENT">
      </member>
      <member name="extended_event" value="14" c:identifier="GST_MPEGTS_DVB_LINKAGE_EXTENDED_EVENT">
      </member>
    </enumeration>
    <record name="DVBParentalRatingItem" c:type="GstMpegtsDVBParentalRatingItem" glib:type-name="GstMpegtsDVBParentalRatingItem" glib:get-type="gst_mpegts_dvb_parental_rating_item_get_type" c:symbol-prefix="dvb_parental_rating_item">
      
      <field name="country_code" writable="1">
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="rating" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
    </record>
    <enumeration name="DVBScramblingModeType" c:type="GstMpegtsDVBScramblingModeType">
      
      <member name="reserved" value="0" c:identifier="GST_MPEGTS_DVB_SCRAMBLING_MODE_RESERVED">
      </member>
      <member name="csa1" value="1" c:identifier="GST_MPEGTS_DVB_SCRAMBLING_MODE_CSA1">
      </member>
      <member name="csa2" value="2" c:identifier="GST_MPEGTS_DVB_SCRAMBLING_MODE_CSA2">
      </member>
      <member name="csa3_standard" value="3" c:identifier="GST_MPEGTS_DVB_SCRAMBLING_MODE_CSA3_STANDARD">
      </member>
      <member name="csa3_minimal_enhanced" value="4" c:identifier="GST_MPEGTS_DVB_SCRAMBLING_MODE_CSA3_MINIMAL_ENHANCED">
      </member>
      <member name="csa3_full_enhanced" value="5" c:identifier="GST_MPEGTS_DVB_SCRAMBLING_MODE_CSA3_FULL_ENHANCED">
      </member>
      <member name="cissa" value="16" c:identifier="GST_MPEGTS_DVB_SCRAMBLING_MODE_CISSA">
      </member>
      <member name="atis_0" value="112" c:identifier="GST_MPEGTS_DVB_SCRAMBLING_MODE_ATIS_0">
      </member>
      <member name="atis_f" value="127" c:identifier="GST_MPEGTS_DVB_SCRAMBLING_MODE_ATIS_F">
      </member>
    </enumeration>
    <record name="DVBServiceListItem" c:type="GstMpegtsDVBServiceListItem" glib:type-name="GstMpegtsDVBServiceListItem" glib:get-type="gst_mpegts_dvb_service_list_item_get_type" c:symbol-prefix="dvb_service_list_item">
      
      <field name="service_id" writable="1">
        <doc xml:space="preserve">the id of a service</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="type" writable="1">
        <doc xml:space="preserve">the type of a service</doc>
        <type name="DVBServiceType" c:type="GstMpegtsDVBServiceType"/>
      </field>
    </record>
    <enumeration name="DVBServiceType" c:type="GstMpegtsDVBServiceType">
      <doc xml:space="preserve">The type of service of a channel.

As specified in Table 87 of ETSI EN 300 468 v1.13.1</doc>
      
      <member name="reserved_00" value="0" c:identifier="GST_DVB_SERVICE_RESERVED_00">
      </member>
      <member name="digital_television" value="1" c:identifier="GST_DVB_SERVICE_DIGITAL_TELEVISION">
      </member>
      <member name="digital_radio_sound" value="2" c:identifier="GST_DVB_SERVICE_DIGITAL_RADIO_SOUND">
      </member>
      <member name="teletext" value="3" c:identifier="GST_DVB_SERVICE_TELETEXT">
      </member>
      <member name="nvod_reference" value="4" c:identifier="GST_DVB_SERVICE_NVOD_REFERENCE">
      </member>
      <member name="nvod_time_shifted" value="5" c:identifier="GST_DVB_SERVICE_NVOD_TIME_SHIFTED">
      </member>
      <member name="mosaic" value="6" c:identifier="GST_DVB_SERVICE_MOSAIC">
      </member>
      <member name="fm_radio" value="7" c:identifier="GST_DVB_SERVICE_FM_RADIO">
      </member>
      <member name="dvb_srm" value="8" c:identifier="GST_DVB_SERVICE_DVB_SRM">
      </member>
      <member name="reserved_09" value="9" c:identifier="GST_DVB_SERVICE_RESERVED_09">
      </member>
      <member name="advanced_codec_digital_radio_sound" value="10" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_DIGITAL_RADIO_SOUND">
      </member>
      <member name="advanced_codec_mosaic" value="11" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_MOSAIC">
      </member>
      <member name="data_broadcast" value="12" c:identifier="GST_DVB_SERVICE_DATA_BROADCAST">
      </member>
      <member name="reserved_0d_common_interface" value="13" c:identifier="GST_DVB_SERVICE_RESERVED_0D_COMMON_INTERFACE">
      </member>
      <member name="rcs_map" value="14" c:identifier="GST_DVB_SERVICE_RCS_MAP">
      </member>
      <member name="rcs_fls" value="15" c:identifier="GST_DVB_SERVICE_RCS_FLS">
      </member>
      <member name="dvb_mhp" value="16" c:identifier="GST_DVB_SERVICE_DVB_MHP">
      </member>
      <member name="mpeg2_hd_digital_television" value="17" c:identifier="GST_DVB_SERVICE_MPEG2_HD_DIGITAL_TELEVISION">
      </member>
      <member name="advanced_codec_sd_digital_television" value="22" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_SD_DIGITAL_TELEVISION">
      </member>
      <member name="advanced_codec_sd_nvod_time_shifted" value="23" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_SD_NVOD_TIME_SHIFTED">
      </member>
      <member name="advanced_codec_sd_nvod_reference" value="24" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_SD_NVOD_REFERENCE">
      </member>
      <member name="advanced_codec_hd_digital_television" value="25" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_HD_DIGITAL_TELEVISION">
      </member>
      <member name="advanced_codec_hd_nvod_time_shifted" value="26" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_HD_NVOD_TIME_SHIFTED">
      </member>
      <member name="advanced_codec_hd_nvod_reference" value="27" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_HD_NVOD_REFERENCE">
      </member>
      <member name="advanced_codec_stereo_hd_digital_television" value="28" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_STEREO_HD_DIGITAL_TELEVISION">
      </member>
      <member name="advanced_codec_stereo_hd_nvod_time_shifted" value="29" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_STEREO_HD_NVOD_TIME_SHIFTED">
      </member>
      <member name="advanced_codec_stereo_hd_nvod_reference" value="30" c:identifier="GST_DVB_SERVICE_ADVANCED_CODEC_STEREO_HD_NVOD_REFERENCE">
      </member>
      <member name="reserved_ff" value="31" c:identifier="GST_DVB_SERVICE_RESERVED_FF">
      </member>
    </enumeration>
    <enumeration name="DVBTeletextType" c:type="GstMpegtsDVBTeletextType">
      <doc xml:space="preserve">The type of teletext page.

As specified in Table 100 of ETSI EN 300 468 v1.13.1</doc>
      
      <member name="nitial_page" value="1" c:identifier="INITIAL_PAGE">
      </member>
      <member name="ubtitle_page" value="2" c:identifier="SUBTITLE_PAGE">
      </member>
      <member name="dditional_info_page" value="3" c:identifier="ADDITIONAL_INFO_PAGE">
      </member>
      <member name="rogramme_schedule_page" value="4" c:identifier="PROGRAMME_SCHEDULE_PAGE">
      </member>
      <member name="earing_impaired_page" value="5" c:identifier="HEARING_IMPAIRED_PAGE">
      </member>
    </enumeration>
    <record name="DataBroadcastDescriptor" c:type="GstMpegtsDataBroadcastDescriptor" glib:type-name="GstMpegtsDataBroadcastDescriptor" glib:get-type="gst_mpegts_dvb_data_broadcast_descriptor_get_type" c:symbol-prefix="dvb_data_broadcast_descriptor">
      
      <field name="data_broadcast_id" writable="1">
        <doc xml:space="preserve">the data broadcast id</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="component_tag" writable="1">
        <doc xml:space="preserve">the component tag</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="length" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="selector_bytes" writable="1">
        <doc xml:space="preserve">the selector byte field</doc>
        <type name="guint8" c:type="guint8*"/>
      </field>
      <field name="language_code" writable="1">
        <doc xml:space="preserve">language of @text</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="text" writable="1">
        <doc xml:space="preserve">description of data broadcast</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
      <method name="free" c:identifier="gst_mpegts_dvb_data_broadcast_descriptor_free">
        
        <return-value transfer-ownership="none">
          <type name="none" c:type="void"/>
        </return-value>
        <parameters>
          <instance-parameter name="source" transfer-ownership="none">
            <type name="DataBroadcastDescriptor" c:type="GstMpegtsDataBroadcastDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
    </record>
    <record name="Descriptor" c:type="GstMpegtsDescriptor" glib:type-name="GstMpegtsDescriptor" glib:get-type="gst_mpegts_descriptor_get_type" c:symbol-prefix="descriptor">
      <doc xml:space="preserve">These are the base descriptor types and methods.

For more details, refer to the ITU H.222.0 or ISO/IEC 13818-1 specifications
and other specifications mentioned in the documentation.</doc>
      
      <field name="tag" writable="1">
        <doc xml:space="preserve">the type of descriptor</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="tag_extension" writable="1">
        <doc xml:space="preserve">the extended type (if @descriptor_tag is 0x7f)</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="length" writable="1">
        <doc xml:space="preserve">the length of the descriptor content (excluding tag/length field)</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="data" writable="1">
        <doc xml:space="preserve">the full descriptor data (including tag, extension, length). The first
two bytes are the @tag and @length.</doc>
        <type name="guint8" c:type="guint8*"/>
      </field>
      <field name="_gst_reserved" readable="0" private="1">
        <array zero-terminated="0" fixed-size="4">
          <type name="gpointer" c:type="gpointer"/>
        </array>
      </field>
      <method name="free" c:identifier="gst_mpegts_descriptor_free">
        <doc xml:space="preserve">Frees @desc</doc>
        
        <return-value transfer-ownership="none">
          <type name="none" c:type="void"/>
        </return-value>
        <parameters>
          <instance-parameter name="desc" transfer-ownership="none">
            <doc xml:space="preserve">The descriptor to free</doc>
            <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="parse_ca" c:identifier="gst_mpegts_descriptor_parse_ca">
        <doc xml:space="preserve">Extracts the Conditional Access information from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_CA #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="ca_system_id" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the type of CA system used</doc>
            <type name="guint16" c:type="guint16*"/>
          </parameter>
          <parameter name="ca_pid" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">The PID containing ECM or EMM data</doc>
            <type name="guint16" c:type="guint16*"/>
          </parameter>
          <parameter name="private_data" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">The private data</doc>
            <array length="3" zero-terminated="0" c:type="const guint8**">
              <type name="guint8" c:type="guint8*"/>
            </array>
          </parameter>
          <parameter name="private_data_size" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">The size of @private_data in bytes</doc>
            <type name="gsize" c:type="gsize*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_cable_delivery_system" c:identifier="gst_mpegts_descriptor_parse_cable_delivery_system">
        <doc xml:space="preserve">Extracts the cable delivery system information from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_CABLE_DELIVERY_SYSTEM #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="res" direction="out" caller-allocates="1" transfer-ownership="none">
            <doc xml:space="preserve">the #GstMpegtsCableDeliverySystemDescriptor to fill</doc>
            <type name="CableDeliverySystemDescriptor" c:type="GstMpegtsCableDeliverySystemDescriptor*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_bouquet_name" c:identifier="gst_mpegts_descriptor_parse_dvb_bouquet_name">
        <doc xml:space="preserve">Extracts the bouquet name from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="bouquet_name" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">the bouquet name</doc>
            <type name="utf8" c:type="gchar**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_ca_identifier" c:identifier="gst_mpegts_descriptor_parse_dvb_ca_identifier">
        <doc xml:space="preserve">Extracts ca id's from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_CA_IDENTIFIER #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="list" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">a list of ca identifier.
Edge entry identifies the CA system. Allocations of the value of this field
are found in http://www.dvbservices.com</doc>
            <array name="GLib.Array" c:type="GArray**">
              <type name="guint16"/>
            </array>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_component" c:identifier="gst_mpegts_descriptor_parse_dvb_component">
        <doc xml:space="preserve">Extracts the DVB component information from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_COMPONENT #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="res" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the #GstMpegtsComponentDescriptor to fill</doc>
            <type name="ComponentDescriptor" c:type="GstMpegtsComponentDescriptor**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_content" c:identifier="gst_mpegts_descriptor_parse_dvb_content">
        <doc xml:space="preserve">Extracts the DVB content information from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_CONTENT #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="content" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">#GstMpegtsContent</doc>
            <array name="GLib.PtrArray" c:type="GPtrArray**">
              <type name="Content"/>
            </array>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_data_broadcast" c:identifier="gst_mpegts_descriptor_parse_dvb_data_broadcast">
        <doc xml:space="preserve">Parses out the data broadcast from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_DATA_BROADCAST #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="res" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">#GstMpegtsDataBroadcastDescriptor</doc>
            <type name="DataBroadcastDescriptor" c:type="GstMpegtsDataBroadcastDescriptor**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_data_broadcast_id" c:identifier="gst_mpegts_descriptor_parse_dvb_data_broadcast_id">
        <doc xml:space="preserve">Parses out the data broadcast id from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_DATA_BROADCAST_ID #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="data_broadcast_id" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the data broadcast id</doc>
            <type name="guint16" c:type="guint16*"/>
          </parameter>
          <parameter name="id_selector_bytes" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the selector bytes, if present</doc>
            <array length="2" zero-terminated="0" c:type="guint8**">
              <type name="guint8" c:type="guint8*"/>
            </array>
          </parameter>
          <parameter name="len" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the length of @id_selector_bytes</doc>
            <type name="guint8" c:type="guint8*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_extended_event" c:identifier="gst_mpegts_descriptor_parse_dvb_extended_event">
        <doc xml:space="preserve">Extracts the DVB extended event information from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_EXTENDED_EVENT #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="res" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the #GstMpegtsExtendedEventDescriptor to fill</doc>
            <type name="ExtendedEventDescriptor" c:type="GstMpegtsExtendedEventDescriptor**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_frequency_list" c:identifier="gst_mpegts_descriptor_parse_dvb_frequency_list">
        <doc xml:space="preserve">Parses out a list of frequencies from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_FREQUENCY_LIST #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="offset" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">%FALSE in Hz, %TRUE in kHz</doc>
            <type name="gboolean" c:type="gboolean*"/>
          </parameter>
          <parameter name="list" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">a list of all frequencies in Hz/kHz
depending on @offset</doc>
            <array name="GLib.Array" c:type="GArray**">
              <type name="guint32"/>
            </array>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_linkage" c:identifier="gst_mpegts_descriptor_parse_dvb_linkage">
        <doc xml:space="preserve">Extracts the DVB linkage information from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_LINKAGE #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="res" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the #GstMpegtsDVBLinkageDescriptor to fill</doc>
            <type name="DVBLinkageDescriptor" c:type="GstMpegtsDVBLinkageDescriptor**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_multilingual_bouquet_name" c:identifier="gst_mpegts_descriptor_parse_dvb_multilingual_bouquet_name">
        <doc xml:space="preserve">Parses out the multilingual bouquet name from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_MULTILINGUAL_BOUQUET_NAME
#GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="bouquet_name_items" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">
a #GstMpegtsDvbMultilingualBouquetNameItem</doc>
            <array name="GLib.PtrArray" c:type="GPtrArray**">
              <type name="DvbMultilingualBouquetNameItem"/>
            </array>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_multilingual_component" c:identifier="gst_mpegts_descriptor_parse_dvb_multilingual_component">
        <doc xml:space="preserve">Parses out the multilingual component from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_MULTILINGUAL_COMPONENT
#GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="component_tag" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the component tag</doc>
            <type name="guint8" c:type="guint8*"/>
          </parameter>
          <parameter name="component_description_items" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">
a #GstMpegtsDvbMultilingualComponentItem</doc>
            <array name="GLib.PtrArray" c:type="GPtrArray**">
              <type name="DvbMultilingualComponentItem"/>
            </array>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_multilingual_network_name" c:identifier="gst_mpegts_descriptor_parse_dvb_multilingual_network_name">
        <doc xml:space="preserve">Parses out the multilingual network name from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_MULTILINGUAL_NETWORK_NAME
#GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="network_name_items" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">
a #GstMpegtsDvbMultilingualNetworkNameItem</doc>
            <array name="GLib.PtrArray" c:type="GPtrArray**">
              <type name="DvbMultilingualNetworkNameItem"/>
            </array>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_multilingual_service_name" c:identifier="gst_mpegts_descriptor_parse_dvb_multilingual_service_name">
        <doc xml:space="preserve">Parses out the multilingual service name from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_MULTILINGUAL_SERVICE_NAME
#GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="service_name_items" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">
a #GstMpegtsDvbMultilingualServiceNameItem</doc>
            <array name="GLib.PtrArray" c:type="GPtrArray**">
              <type name="DvbMultilingualServiceNameItem"/>
            </array>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_network_name" c:identifier="gst_mpegts_descriptor_parse_dvb_network_name">
        <doc xml:space="preserve">Parses out the dvb network name from the @descriptor:</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_NETWORK_NAME #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="name" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the extracted name</doc>
            <type name="utf8" c:type="gchar**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_parental_rating" c:identifier="gst_mpegts_descriptor_parse_dvb_parental_rating">
        <doc xml:space="preserve">Extracts the DVB parental rating information from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_PARENTAL_RATING #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="rating" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">
#GstMpegtsDVBParentalRatingItem</doc>
            <array name="GLib.PtrArray" c:type="GPtrArray**">
              <type name="DVBParentalRatingItem"/>
            </array>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_private_data_specifier" c:identifier="gst_mpegts_descriptor_parse_dvb_private_data_specifier">
        <doc xml:space="preserve">Parses out the private data specifier from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_PRIVATE_DATA_SPECIFIER #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="private_data_specifier" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the private data specifier id
registered by http://www.dvbservices.com/</doc>
            <type name="guint32" c:type="guint32*"/>
          </parameter>
          <parameter name="private_data" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">additional data or NULL</doc>
            <array length="2" zero-terminated="0" c:type="guint8**">
              <type name="guint8" c:type="guint8*"/>
            </array>
          </parameter>
          <parameter name="length" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">length of @private_data</doc>
            <type name="guint8" c:type="guint8*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_scrambling" c:identifier="gst_mpegts_descriptor_parse_dvb_scrambling">
        <doc xml:space="preserve">Parses out the scrambling mode from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_SCRAMBLING #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="scrambling_mode" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">This 8-bit field identifies the selected
mode of the scrambling algorithm (#GstMpegtsDVBScramblingModeType).
The technical details of the scrambling algorithm are available only
to bona-fide users upon signature of a Non Disclosure Agreement (NDA)
administered by the DVB Common Scrambling Algorithm Custodian.</doc>
            <type name="DVBScramblingModeType" c:type="GstMpegtsDVBScramblingModeType*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_service" c:identifier="gst_mpegts_descriptor_parse_dvb_service">
        <doc xml:space="preserve">Extracts the dvb service information from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_SERVICE #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="service_type" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">the service type</doc>
            <type name="DVBServiceType" c:type="GstMpegtsDVBServiceType*"/>
          </parameter>
          <parameter name="service_name" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">the service name</doc>
            <type name="utf8" c:type="gchar**"/>
          </parameter>
          <parameter name="provider_name" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">the provider name</doc>
            <type name="utf8" c:type="gchar**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_service_list" c:identifier="gst_mpegts_descriptor_parse_dvb_service_list">
        <doc xml:space="preserve">Parses out a list of services from the @descriptor:</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_SERVICE_LIST #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="list" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">
the list of services</doc>
            <array name="GLib.PtrArray" c:type="GPtrArray**">
              <type name="DVBServiceListItem"/>
            </array>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_short_event" c:identifier="gst_mpegts_descriptor_parse_dvb_short_event">
        <doc xml:space="preserve">Extracts the DVB short event information from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_SHORT_EVENT #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="language_code" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">the language code</doc>
            <type name="utf8" c:type="gchar**"/>
          </parameter>
          <parameter name="event_name" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">the event name</doc>
            <type name="utf8" c:type="gchar**"/>
          </parameter>
          <parameter name="text" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">the event text</doc>
            <type name="utf8" c:type="gchar**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_stream_identifier" c:identifier="gst_mpegts_descriptor_parse_dvb_stream_identifier">
        <doc xml:space="preserve">Extracts the component tag from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_CONTENT #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="component_tag" direction="out" caller-allocates="0" transfer-ownership="none">
            <doc xml:space="preserve">the component tag</doc>
            <type name="guint8" c:type="guint8*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_stuffing" c:identifier="gst_mpegts_descriptor_parse_dvb_stuffing">
        <doc xml:space="preserve">Parses out the stuffing bytes from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_STUFFING #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="stuffing_bytes" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the stuffing bytes</doc>
            <type name="guint8" c:type="guint8**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_subtitling_idx" c:identifier="gst_mpegts_descriptor_parse_dvb_subtitling_idx">
        <doc xml:space="preserve">Extracts the DVB subtitling informatio from specific table id in @descriptor.

Note: Use #gst_tag_get_language_code if you want to get the the
ISO 639-1 language code from the returned ISO 639-2 one.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_SUBTITLING #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="idx" transfer-ownership="none">
            <doc xml:space="preserve">Table id of the entry to parse</doc>
            <type name="guint" c:type="guint"/>
          </parameter>
          <parameter name="lang" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the language code</doc>
            <type name="utf8" c:type="gchar**"/>
          </parameter>
          <parameter name="type" direction="out" caller-allocates="0" transfer-ownership="none" optional="1" allow-none="1">
            <doc xml:space="preserve">the type of subtitling</doc>
            <type name="guint8" c:type="guint8*"/>
          </parameter>
          <parameter name="composition_page_id" direction="out" caller-allocates="0" transfer-ownership="none" optional="1" allow-none="1">
            <doc xml:space="preserve">the composition page id</doc>
            <type name="guint16" c:type="guint16*"/>
          </parameter>
          <parameter name="ancillary_page_id" direction="out" caller-allocates="0" transfer-ownership="none" optional="1" allow-none="1">
            <doc xml:space="preserve">the ancillary page id</doc>
            <type name="guint16" c:type="guint16*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_subtitling_nb" c:identifier="gst_mpegts_descriptor_parse_dvb_subtitling_nb">
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The number of entries in @descriptor</doc>
          <type name="guint" c:type="guint"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_SUBTITLING #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="parse_dvb_t2_delivery_system" c:identifier="gst_mpegts_descriptor_parse_dvb_t2_delivery_system">
        <doc xml:space="preserve">Parses out the DVB-T2 delivery system from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_EXT_DVB_T2_DELIVERY_SYSTEM #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="res" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">#GstMpegtsT2DeliverySystemDescriptor</doc>
            <type name="T2DeliverySystemDescriptor" c:type="GstMpegtsT2DeliverySystemDescriptor**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_teletext_idx" c:identifier="gst_mpegts_descriptor_parse_dvb_teletext_idx">
        <doc xml:space="preserve">Parses teletext number @idx in the @descriptor. The language is in ISO639 format.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">FALSE on out-of-bounds and errors</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_TELETEXT #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="idx" transfer-ownership="none">
            <doc xml:space="preserve">The id of the teletext to get</doc>
            <type name="guint" c:type="guint"/>
          </parameter>
          <parameter name="language_code" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">a null-terminated string</doc>
            <type name="utf8" c:type="gchar**"/>
          </parameter>
          <parameter name="teletext_type" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <doc xml:space="preserve">#GstMpegtsDVBTeletextType</doc>
            <type name="DVBTeletextType" c:type="GstMpegtsDVBTeletextType*"/>
          </parameter>
          <parameter name="magazine_number" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <type name="guint8" c:type="guint8*"/>
          </parameter>
          <parameter name="page_number" direction="out" caller-allocates="0" transfer-ownership="full" optional="1" allow-none="1">
            <type name="guint8" c:type="guint8*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_dvb_teletext_nb" c:identifier="gst_mpegts_descriptor_parse_dvb_teletext_nb">
        <doc xml:space="preserve">Find the number of teletext entries in @descriptor</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">Number of teletext entries</doc>
          <type name="guint" c:type="guint"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_TELETEXT #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="parse_iso_639_language" c:identifier="gst_mpegts_descriptor_parse_iso_639_language">
        <doc xml:space="preserve">Extracts the iso 639-2 language information from @descriptor.

Note: Use #gst_tag_get_language_code if you want to get the the
ISO 639-1 language code from the returned ISO 639-2 one.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_ISO_639_LANGUAGE #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="res" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">the #GstMpegtsISO639LanguageDescriptor to fill</doc>
            <type name="ISO639LanguageDescriptor" c:type="GstMpegtsISO639LanguageDescriptor**"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_iso_639_language_idx" c:identifier="gst_mpegts_descriptor_parse_iso_639_language_idx">
        <doc xml:space="preserve">Extracts the iso 639-2 language information from specific table id in @descriptor.

Note: Use #gst_tag_get_language_code if you want to get the the
ISO 639-1 language code from the returned ISO 639-2 one.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_ISO_639_LANGUAGE #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="idx" transfer-ownership="none">
            <doc xml:space="preserve">Table id of the language to parse</doc>
            <type name="guint" c:type="guint"/>
          </parameter>
          <parameter name="lang" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">4-byte gchar array to hold the language code</doc>
            <type name="utf8" c:type="gchar**"/>
          </parameter>
          <parameter name="audio_type" direction="out" caller-allocates="0" transfer-ownership="none" optional="1" allow-none="1">
            <doc xml:space="preserve">the #GstMpegtsIso639AudioType to set</doc>
            <type name="Iso639AudioType" c:type="GstMpegtsIso639AudioType*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_iso_639_language_nb" c:identifier="gst_mpegts_descriptor_parse_iso_639_language_nb">
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The number of languages in @descriptor</doc>
          <type name="guint" c:type="guint"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_ISO_639_LANGUAGE #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="parse_logical_channel" c:identifier="gst_mpegts_descriptor_parse_logical_channel">
        <doc xml:space="preserve">Extracts the logical channels from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DTG_LOGICAL_CHANNEL #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="res" direction="out" caller-allocates="1" transfer-ownership="none">
            <doc xml:space="preserve">the #GstMpegtsLogicalChannelDescriptor to fill</doc>
            <type name="LogicalChannelDescriptor" c:type="GstMpegtsLogicalChannelDescriptor*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_satellite_delivery_system" c:identifier="gst_mpegts_descriptor_parse_satellite_delivery_system">
        <doc xml:space="preserve">Extracts the satellite delivery system information from @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if parsing succeeded, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_SATELLITE_DELIVERY_SYSTEM #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="res" direction="out" caller-allocates="1" transfer-ownership="none">
            <doc xml:space="preserve">the #GstMpegtsSatelliteDeliverySystemDescriptor to fill</doc>
            <type name="SatelliteDeliverySystemDescriptor" c:type="GstMpegtsSatelliteDeliverySystemDescriptor*"/>
          </parameter>
        </parameters>
      </method>
      <method name="parse_terrestrial_delivery_system" c:identifier="gst_mpegts_descriptor_parse_terrestrial_delivery_system">
        <doc xml:space="preserve">Parses out the terrestrial delivery system from the @descriptor.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the parsing happened correctly, else %FALSE.</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="descriptor" transfer-ownership="none">
            <doc xml:space="preserve">a %GST_MTS_DESC_DVB_TERRESTRIAL_DELIVERY_SYSTEM #GstMpegtsDescriptor</doc>
            <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
          </instance-parameter>
          <parameter name="res" direction="out" caller-allocates="1" transfer-ownership="none">
            <doc xml:space="preserve">#GstMpegtsTerrestrialDeliverySystemDescriptor</doc>
            <type name="TerrestrialDeliverySystemDescriptor" c:type="GstMpegtsTerrestrialDeliverySystemDescriptor*"/>
          </parameter>
        </parameters>
      </method>
      <function name="from_custom" c:identifier="gst_mpegts_descriptor_from_custom">
        <doc xml:space="preserve">Creates a #GstMpegtsDescriptor with custom @tag and @data</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">#GstMpegtsDescriptor</doc>
          <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
        </return-value>
        <parameters>
          <parameter name="tag" transfer-ownership="none">
            <doc xml:space="preserve">descriptor tag</doc>
            <type name="guint8" c:type="guint8"/>
          </parameter>
          <parameter name="data" transfer-ownership="none">
            <doc xml:space="preserve">descriptor data (after tag and length field)</doc>
            <array length="2" zero-terminated="0" c:type="const guint8*">
              <type name="guint8" c:type="guint8"/>
            </array>
          </parameter>
          <parameter name="length" transfer-ownership="none">
            <doc xml:space="preserve">length of @data</doc>
            <type name="gsize" c:type="gsize"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_custom_with_extension" c:identifier="gst_mpegts_descriptor_from_custom_with_extension">
        <doc xml:space="preserve">Creates a #GstMpegtsDescriptor with custom @tag, @tag_extension and @data</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">#GstMpegtsDescriptor</doc>
          <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
        </return-value>
        <parameters>
          <parameter name="tag" transfer-ownership="none">
            <doc xml:space="preserve">descriptor tag</doc>
            <type name="guint8" c:type="guint8"/>
          </parameter>
          <parameter name="tag_extension" transfer-ownership="none">
            <doc xml:space="preserve">descriptor tag extension</doc>
            <type name="guint8" c:type="guint8"/>
          </parameter>
          <parameter name="data" transfer-ownership="none">
            <doc xml:space="preserve">descriptor data (after tag and length field)</doc>
            <array length="3" zero-terminated="0" c:type="const guint8*">
              <type name="guint8" c:type="guint8"/>
            </array>
          </parameter>
          <parameter name="length" transfer-ownership="none">
            <doc xml:space="preserve">length of @data</doc>
            <type name="gsize" c:type="gsize"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_dvb_network_name" c:identifier="gst_mpegts_descriptor_from_dvb_network_name">
        <doc xml:space="preserve">Creates a #GstMpegtsDescriptor to be a %GST_MTS_DESC_DVB_NETWORK_NAME,
with the network name @name. The data field of the #GstMpegtsDescriptor
will be allocated, and transferred to the caller.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">the #GstMpegtsDescriptor or %NULL on fail</doc>
          <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
        </return-value>
        <parameters>
          <parameter name="name" transfer-ownership="none">
            <doc xml:space="preserve">the network name to set</doc>
            <type name="utf8" c:type="const gchar*"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_dvb_service" c:identifier="gst_mpegts_descriptor_from_dvb_service">
        <doc xml:space="preserve">Fills a #GstMpegtsDescriptor to be a %GST_MTS_DESC_DVB_SERVICE.
The data field of the #GstMpegtsDescriptor will be allocated,
and transferred to the caller.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">the #GstMpegtsDescriptor or %NULL on fail</doc>
          <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
        </return-value>
        <parameters>
          <parameter name="service_type" transfer-ownership="none">
            <doc xml:space="preserve">Service type defined as a #GstMpegtsDVBServiceType</doc>
            <type name="DVBServiceType" c:type="GstMpegtsDVBServiceType"/>
          </parameter>
          <parameter name="service_name" transfer-ownership="none" nullable="1" allow-none="1">
            <doc xml:space="preserve">Name of the service</doc>
            <type name="utf8" c:type="const gchar*"/>
          </parameter>
          <parameter name="service_provider" transfer-ownership="none" nullable="1" allow-none="1">
            <doc xml:space="preserve">Name of the service provider</doc>
            <type name="utf8" c:type="const gchar*"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_dvb_subtitling" c:identifier="gst_mpegts_descriptor_from_dvb_subtitling">
        
        <return-value transfer-ownership="full">
          <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
        </return-value>
        <parameters>
          <parameter name="lang" transfer-ownership="none">
            <doc xml:space="preserve">a string containing the ISO639 language</doc>
            <type name="utf8" c:type="const gchar*"/>
          </parameter>
          <parameter name="type" transfer-ownership="none">
            <doc xml:space="preserve">subtitling type</doc>
            <type name="guint8" c:type="guint8"/>
          </parameter>
          <parameter name="composition" transfer-ownership="none">
            <doc xml:space="preserve">composition page id</doc>
            <type name="guint16" c:type="guint16"/>
          </parameter>
          <parameter name="ancillary" transfer-ownership="none">
            <doc xml:space="preserve">ancillary page id</doc>
            <type name="guint16" c:type="guint16"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_iso_639_language" c:identifier="gst_mpegts_descriptor_from_iso_639_language">
        <doc xml:space="preserve">Creates a %GST_MTS_DESC_ISO_639_LANGUAGE #GstMpegtsDescriptor with
a single language</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">#GstMpegtsDescriptor, %NULL on failure</doc>
          <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
        </return-value>
        <parameters>
          <parameter name="language" transfer-ownership="none">
            <doc xml:space="preserve">ISO-639-2 language 3-char code</doc>
            <type name="utf8" c:type="const gchar*"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_registration" c:identifier="gst_mpegts_descriptor_from_registration">
        <doc xml:space="preserve">Creates a %GST_MTS_DESC_REGISTRATION #GstMpegtsDescriptor</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">#GstMpegtsDescriptor, %NULL on failure</doc>
          <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
        </return-value>
        <parameters>
          <parameter name="format_identifier" transfer-ownership="none">
            <doc xml:space="preserve">a 4 character format identifier string</doc>
            <type name="utf8" c:type="const gchar*"/>
          </parameter>
          <parameter name="additional_info" transfer-ownership="none" nullable="1" allow-none="1">
            <doc xml:space="preserve">pointer to optional additional info</doc>
            <array length="2" zero-terminated="0" c:type="guint8*">
              <type name="guint8" c:type="guint8"/>
            </array>
          </parameter>
          <parameter name="additional_info_length" transfer-ownership="none">
            <doc xml:space="preserve">length of the optional @additional_info</doc>
            <type name="gsize" c:type="gsize"/>
          </parameter>
        </parameters>
      </function>
    </record>
    <enumeration name="DescriptorType" c:type="GstMpegtsDescriptorType">
      <doc xml:space="preserve">The type of #GstMpegtsDescriptor

These values correspond to the registered descriptor type from
the base MPEG-TS specifications (ITU H.222.0 | ISO/IEC 13818-1).

Consult the relevant specifications for more details.</doc>
      
      <member name="reserved_00" value="0" c:identifier="GST_MTS_DESC_RESERVED_00">
      </member>
      <member name="reserved_01" value="1" c:identifier="GST_MTS_DESC_RESERVED_01">
      </member>
      <member name="video_stream" value="2" c:identifier="GST_MTS_DESC_VIDEO_STREAM">
      </member>
      <member name="audio_stream" value="3" c:identifier="GST_MTS_DESC_AUDIO_STREAM">
      </member>
      <member name="hierarchy" value="4" c:identifier="GST_MTS_DESC_HIERARCHY">
      </member>
      <member name="registration" value="5" c:identifier="GST_MTS_DESC_REGISTRATION">
      </member>
      <member name="data_stream_alignment" value="6" c:identifier="GST_MTS_DESC_DATA_STREAM_ALIGNMENT">
      </member>
      <member name="target_background_grid" value="7" c:identifier="GST_MTS_DESC_TARGET_BACKGROUND_GRID">
      </member>
      <member name="video_window" value="8" c:identifier="GST_MTS_DESC_VIDEO_WINDOW">
      </member>
      <member name="ca" value="9" c:identifier="GST_MTS_DESC_CA">
      </member>
      <member name="iso_639_language" value="10" c:identifier="GST_MTS_DESC_ISO_639_LANGUAGE">
      </member>
      <member name="system_clock" value="11" c:identifier="GST_MTS_DESC_SYSTEM_CLOCK">
      </member>
      <member name="multiplex_buffer_utilisation" value="12" c:identifier="GST_MTS_DESC_MULTIPLEX_BUFFER_UTILISATION">
      </member>
      <member name="copyright" value="13" c:identifier="GST_MTS_DESC_COPYRIGHT">
      </member>
      <member name="maximum_bitrate" value="14" c:identifier="GST_MTS_DESC_MAXIMUM_BITRATE">
      </member>
      <member name="private_data_indicator" value="15" c:identifier="GST_MTS_DESC_PRIVATE_DATA_INDICATOR">
      </member>
      <member name="smoothing_buffer" value="16" c:identifier="GST_MTS_DESC_SMOOTHING_BUFFER">
      </member>
      <member name="std" value="17" c:identifier="GST_MTS_DESC_STD">
      </member>
      <member name="ibp" value="18" c:identifier="GST_MTS_DESC_IBP">
      </member>
      <member name="dsmcc_carousel_identifier" value="19" c:identifier="GST_MTS_DESC_DSMCC_CAROUSEL_IDENTIFIER">
      </member>
      <member name="dsmcc_association_tag" value="20" c:identifier="GST_MTS_DESC_DSMCC_ASSOCIATION_TAG">
      </member>
      <member name="dsmcc_deferred_association_tag" value="21" c:identifier="GST_MTS_DESC_DSMCC_DEFERRED_ASSOCIATION_TAG">
      </member>
      <member name="dsmcc_npt_reference" value="23" c:identifier="GST_MTS_DESC_DSMCC_NPT_REFERENCE">
      </member>
      <member name="dsmcc_npt_endpoint" value="24" c:identifier="GST_MTS_DESC_DSMCC_NPT_ENDPOINT">
      </member>
      <member name="dsmcc_stream_mode" value="25" c:identifier="GST_MTS_DESC_DSMCC_STREAM_MODE">
      </member>
      <member name="dsmcc_stream_event" value="26" c:identifier="GST_MTS_DESC_DSMCC_STREAM_EVENT">
      </member>
      <member name="mpeg4_video" value="27" c:identifier="GST_MTS_DESC_MPEG4_VIDEO">
      </member>
      <member name="mpeg4_audio" value="28" c:identifier="GST_MTS_DESC_MPEG4_AUDIO">
      </member>
      <member name="iod" value="29" c:identifier="GST_MTS_DESC_IOD">
      </member>
      <member name="sl" value="30" c:identifier="GST_MTS_DESC_SL">
      </member>
      <member name="fmc" value="31" c:identifier="GST_MTS_DESC_FMC">
      </member>
      <member name="external_es_id" value="32" c:identifier="GST_MTS_DESC_EXTERNAL_ES_ID">
      </member>
      <member name="mux_code" value="33" c:identifier="GST_MTS_DESC_MUX_CODE">
      </member>
      <member name="fmx_buffer_size" value="34" c:identifier="GST_MTS_DESC_FMX_BUFFER_SIZE">
      </member>
      <member name="multiplex_buffer" value="35" c:identifier="GST_MTS_DESC_MULTIPLEX_BUFFER">
      </member>
      <member name="content_labeling" value="36" c:identifier="GST_MTS_DESC_CONTENT_LABELING">
      </member>
      <member name="metadata_pointer" value="37" c:identifier="GST_MTS_DESC_METADATA_POINTER">
      </member>
      <member name="metadata" value="38" c:identifier="GST_MTS_DESC_METADATA">
      </member>
      <member name="metadata_std" value="39" c:identifier="GST_MTS_DESC_METADATA_STD">
      </member>
      <member name="avc_video" value="40" c:identifier="GST_MTS_DESC_AVC_VIDEO">
      </member>
      <member name="ipmp" value="41" c:identifier="GST_MTS_DESC_IPMP">
      </member>
      <member name="avc_timing_and_hrd" value="42" c:identifier="GST_MTS_DESC_AVC_TIMING_AND_HRD">
      </member>
      <member name="mpeg2_aac_audio" value="43" c:identifier="GST_MTS_DESC_MPEG2_AAC_AUDIO">
      </member>
      <member name="flex_mux_timing" value="44" c:identifier="GST_MTS_DESC_FLEX_MUX_TIMING">
      </member>
      <member name="mpeg4_text" value="45" c:identifier="GST_MTS_DESC_MPEG4_TEXT">
      </member>
      <member name="mpeg4_audio_extension" value="46" c:identifier="GST_MTS_DESC_MPEG4_AUDIO_EXTENSION">
      </member>
      <member name="auxiliary_video_stream" value="47" c:identifier="GST_MTS_DESC_AUXILIARY_VIDEO_STREAM">
      </member>
      <member name="svc_extension" value="48" c:identifier="GST_MTS_DESC_SVC_EXTENSION">
      </member>
      <member name="mvc_extension" value="49" c:identifier="GST_MTS_DESC_MVC_EXTENSION">
      </member>
      <member name="j2k_video" value="50" c:identifier="GST_MTS_DESC_J2K_VIDEO">
      </member>
      <member name="mvc_operation_point" value="51" c:identifier="GST_MTS_DESC_MVC_OPERATION_POINT">
      </member>
      <member name="mpeg2_stereoscopic_video_format" value="52" c:identifier="GST_MTS_DESC_MPEG2_STEREOSCOPIC_VIDEO_FORMAT">
      </member>
      <member name="stereoscopic_program_info" value="53" c:identifier="GST_MTS_DESC_STEREOSCOPIC_PROGRAM_INFO">
      </member>
      <member name="stereoscopic_video_info" value="54" c:identifier="GST_MTS_DESC_STEREOSCOPIC_VIDEO_INFO">
      </member>
    </enumeration>
    <record name="DvbMultilingualBouquetNameItem" c:type="GstMpegtsDvbMultilingualBouquetNameItem" glib:type-name="GstMpegtsDvbMultilingualBouquetNameItem" glib:get-type="gst_mpegts_dvb_multilingual_bouquet_name_item_get_type" c:symbol-prefix="dvb_multilingual_bouquet_name_item">
      <doc xml:space="preserve">a multilingual bouquet name entry</doc>
      
      <field name="language_code" writable="1">
        <doc xml:space="preserve">the ISO 639 language code</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="bouquet_name" writable="1">
        <doc xml:space="preserve">the bouquet name</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
    </record>
    <record name="DvbMultilingualComponentItem" c:type="GstMpegtsDvbMultilingualComponentItem" glib:type-name="GstMpegtsDvbMultilingualComponentItem" glib:get-type="gst_mpegts_dvb_multilingual_component_item_get_type" c:symbol-prefix="dvb_multilingual_component_item">
      
      <field name="language_code" writable="1">
        <doc xml:space="preserve">the ISO 639 language code</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="description" writable="1">
        <doc xml:space="preserve">the component description</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
    </record>
    <record name="DvbMultilingualNetworkNameItem" c:type="GstMpegtsDvbMultilingualNetworkNameItem" glib:type-name="GstMpegtsDvbMultilingualNetworkNameItem" glib:get-type="gst_mpegts_dvb_multilingual_network_name_item_get_type" c:symbol-prefix="dvb_multilingual_network_name_item">
      <doc xml:space="preserve">a multilingual network name entry</doc>
      
      <field name="language_code" writable="1">
        <doc xml:space="preserve">the ISO 639 language code</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="network_name" writable="1">
        <doc xml:space="preserve">the network name</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
    </record>
    <record name="DvbMultilingualServiceNameItem" c:type="GstMpegtsDvbMultilingualServiceNameItem" glib:type-name="GstMpegtsDvbMultilingualServiceNameItem" glib:get-type="gst_mpegts_dvb_multilingual_service_name_item_get_type" c:symbol-prefix="dvb_multilingual_service_name_item">
      <doc xml:space="preserve">a multilingual service name entry</doc>
      
      <field name="language_code" writable="1">
        <doc xml:space="preserve">the ISO 639 language code</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="provider_name" writable="1">
        <doc xml:space="preserve">the provider name</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="service_name" writable="1">
        <doc xml:space="preserve">the service name</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
    </record>
    <record name="EIT" c:type="GstMpegtsEIT" glib:type-name="GstMpegtsEIT" glib:get-type="gst_mpegts_eit_get_type" c:symbol-prefix="eit">
      <doc xml:space="preserve">Event Information Table (EN 300 468)</doc>
      
      <field name="transport_stream_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="original_network_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="segment_last_section_number" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="last_table_id" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="actual_stream" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="present_following" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="events" writable="1">
        <doc xml:space="preserve">List of events</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="EITEvent"/>
        </array>
      </field>
    </record>
    <record name="EITEvent" c:type="GstMpegtsEITEvent" glib:type-name="GstMpegtsEITEvent" glib:get-type="gst_mpegts_eit_event_get_type" c:symbol-prefix="eit_event">
      <doc xml:space="preserve">Event from a @GstMpegtsEIT</doc>
      
      <field name="event_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="start_time" writable="1">
        <type name="Gst.DateTime" c:type="GstDateTime*"/>
      </field>
      <field name="duration" writable="1">
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="running_status" writable="1">
        <type name="RunningStatus" c:type="GstMpegtsRunningStatus"/>
      </field>
      <field name="free_CA_mode" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">List of descriptors</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
    </record>
    <record name="ExtendedEventDescriptor" c:type="GstMpegtsExtendedEventDescriptor" glib:type-name="GstMpegtsExtendedEventDescriptor" glib:get-type="gst_mpegts_extended_event_descriptor_get_type" c:symbol-prefix="extended_event_descriptor">
      <doc xml:space="preserve">Extended Event Descriptor (EN 300 468 v.1.13.1)</doc>
      
      <field name="descriptor_number" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="last_descriptor_number" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="language_code" writable="1">
        <doc xml:space="preserve">NULL terminated language code.</doc>
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="items" writable="1">
        <doc xml:space="preserve">the #GstMpegtsExtendedEventItem</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="ExtendedEventItem"/>
        </array>
      </field>
      <field name="text" writable="1">
        <type name="utf8" c:type="gchar*"/>
      </field>
      <method name="free" c:identifier="gst_mpegts_extended_event_descriptor_free">
        
        <return-value transfer-ownership="none">
          <type name="none" c:type="void"/>
        </return-value>
        <parameters>
          <instance-parameter name="source" transfer-ownership="none">
            <type name="ExtendedEventDescriptor" c:type="GstMpegtsExtendedEventDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
    </record>
    <record name="ExtendedEventItem" c:type="GstMpegtsExtendedEventItem" glib:type-name="GstMpegtsExtendedEventItem" glib:get-type="gst_mpegts_extended_event_item_get_type" c:symbol-prefix="extended_event_item">
      
      <field name="item_description" writable="1">
        <type name="utf8" c:type="gchar*"/>
      </field>
      <field name="item" writable="1">
        <type name="utf8" c:type="gchar*"/>
      </field>
    </record>
    <enumeration name="ISDBDescriptorType" c:type="GstMpegtsISDBDescriptorType">
      <doc xml:space="preserve">These values correspond to the registered descriptor type from
the various ISDB specifications.

Consult the relevant specifications for more details.</doc>
      
      <member name="hierarchical_transmission" value="192" c:identifier="GST_MTS_DESC_ISDB_HIERARCHICAL_TRANSMISSION">
      </member>
      <member name="digital_copy_control" value="193" c:identifier="GST_MTS_DESC_ISDB_DIGITAL_COPY_CONTROL">
      </member>
      <member name="network_identification" value="194" c:identifier="GST_MTS_DESC_ISDB_NETWORK_IDENTIFICATION">
      </member>
      <member name="partial_ts_time" value="195" c:identifier="GST_MTS_DESC_ISDB_PARTIAL_TS_TIME">
      </member>
      <member name="audio_component" value="196" c:identifier="GST_MTS_DESC_ISDB_AUDIO_COMPONENT">
      </member>
      <member name="hyperlink" value="197" c:identifier="GST_MTS_DESC_ISDB_HYPERLINK">
      </member>
      <member name="target_region" value="198" c:identifier="GST_MTS_DESC_ISDB_TARGET_REGION">
      </member>
      <member name="data_content" value="199" c:identifier="GST_MTS_DESC_ISDB_DATA_CONTENT">
      </member>
      <member name="video_decode_control" value="200" c:identifier="GST_MTS_DESC_ISDB_VIDEO_DECODE_CONTROL">
      </member>
      <member name="download_content" value="201" c:identifier="GST_MTS_DESC_ISDB_DOWNLOAD_CONTENT">
      </member>
      <member name="ca_emm_ts" value="202" c:identifier="GST_MTS_DESC_ISDB_CA_EMM_TS">
      </member>
      <member name="ca_contract_information" value="203" c:identifier="GST_MTS_DESC_ISDB_CA_CONTRACT_INFORMATION">
      </member>
      <member name="ca_service" value="204" c:identifier="GST_MTS_DESC_ISDB_CA_SERVICE">
      </member>
      <member name="ts_information" value="205" c:identifier="GST_MTS_DESC_ISDB_TS_INFORMATION">
      </member>
      <member name="extended_broadcaster" value="206" c:identifier="GST_MTS_DESC_ISDB_EXTENDED_BROADCASTER">
      </member>
      <member name="logo_transmission" value="207" c:identifier="GST_MTS_DESC_ISDB_LOGO_TRANSMISSION">
      </member>
      <member name="basic_local_event" value="208" c:identifier="GST_MTS_DESC_ISDB_BASIC_LOCAL_EVENT">
      </member>
      <member name="reference" value="209" c:identifier="GST_MTS_DESC_ISDB_REFERENCE">
      </member>
      <member name="node_relation" value="210" c:identifier="GST_MTS_DESC_ISDB_NODE_RELATION">
      </member>
      <member name="short_node_information" value="211" c:identifier="GST_MTS_DESC_ISDB_SHORT_NODE_INFORMATION">
      </member>
      <member name="stc_reference" value="212" c:identifier="GST_MTS_DESC_ISDB_STC_REFERENCE">
      </member>
      <member name="series" value="213" c:identifier="GST_MTS_DESC_ISDB_SERIES">
      </member>
      <member name="event_group" value="214" c:identifier="GST_MTS_DESC_ISDB_EVENT_GROUP">
      </member>
      <member name="si_parameter" value="215" c:identifier="GST_MTS_DESC_ISDB_SI_PARAMETER">
      </member>
      <member name="broadcaster_name" value="216" c:identifier="GST_MTS_DESC_ISDB_BROADCASTER_NAME">
      </member>
      <member name="component_group" value="217" c:identifier="GST_MTS_DESC_ISDB_COMPONENT_GROUP">
      </member>
      <member name="si_prime_ts" value="218" c:identifier="GST_MTS_DESC_ISDB_SI_PRIME_TS">
      </member>
      <member name="board_information" value="219" c:identifier="GST_MTS_DESC_ISDB_BOARD_INFORMATION">
      </member>
      <member name="ldt_linkage" value="220" c:identifier="GST_MTS_DESC_ISDB_LDT_LINKAGE">
      </member>
      <member name="connected_transmission" value="221" c:identifier="GST_MTS_DESC_ISDB_CONNECTED_TRANSMISSION">
      </member>
      <member name="content_availability" value="222" c:identifier="GST_MTS_DESC_ISDB_CONTENT_AVAILABILITY">
      </member>
      <member name="service_group" value="224" c:identifier="GST_MTS_DESC_ISDB_SERVICE_GROUP">
      </member>
    </enumeration>
    <record name="ISO639LanguageDescriptor" c:type="GstMpegtsISO639LanguageDescriptor" glib:type-name="GstMpegtsISO639LanguageDescriptor" glib:get-type="gst_mpegts_iso_639_language_get_type" c:symbol-prefix="iso_639_language">
      
      <field name="nb_language" writable="1">
        <type name="guint" c:type="guint"/>
      </field>
      <field name="language" writable="1">
        <array zero-terminated="0" fixed-size="64" c:type="gchar">
          <type name="utf8" c:type="gchar*"/>
        </array>
      </field>
      <field name="audio_type" writable="1">
        <array zero-terminated="0" fixed-size="64">
          <type name="Iso639AudioType" c:type="GstMpegtsIso639AudioType"/>
        </array>
      </field>
      <method name="descriptor_free" c:identifier="gst_mpegts_iso_639_language_descriptor_free">
        
        <return-value transfer-ownership="none">
          <type name="none" c:type="void"/>
        </return-value>
        <parameters>
          <instance-parameter name="desc" transfer-ownership="none">
            <type name="ISO639LanguageDescriptor" c:type="GstMpegtsISO639LanguageDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
    </record>
    <enumeration name="Iso639AudioType" c:type="GstMpegtsIso639AudioType">
      
      <member name="undefined" value="0" c:identifier="GST_MPEGTS_AUDIO_TYPE_UNDEFINED">
      </member>
      <member name="clean_effects" value="1" c:identifier="GST_MPEGTS_AUDIO_TYPE_CLEAN_EFFECTS">
      </member>
      <member name="hearing_impaired" value="2" c:identifier="GST_MPEGTS_AUDIO_TYPE_HEARING_IMPAIRED">
      </member>
      <member name="visual_impaired_commentary" value="3" c:identifier="GST_MPEGTS_AUDIO_TYPE_VISUAL_IMPAIRED_COMMENTARY">
      </member>
    </enumeration>
    <record name="LogicalChannel" c:type="GstMpegtsLogicalChannel" glib:type-name="GstMpegtsLogicalChannel" glib:get-type="gst_mpegts_logical_channel_get_type" c:symbol-prefix="logical_channel">
      
      <field name="service_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="visible_service" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="logical_channel_number" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
    </record>
    <record name="LogicalChannelDescriptor" c:type="GstMpegtsLogicalChannelDescriptor" glib:type-name="GstMpegtsLogicalChannelDescriptor" glib:get-type="gst_mpegts_logical_channel_descriptor_get_type" c:symbol-prefix="logical_channel_descriptor">
      
      <field name="nb_channels" writable="1">
        <type name="guint" c:type="guint"/>
      </field>
      <field name="channels" writable="1">
        <array zero-terminated="0" fixed-size="64">
          <type name="LogicalChannel" c:type="GstMpegtsLogicalChannel"/>
        </array>
      </field>
    </record>
    <enumeration name="MiscDescriptorType" c:type="GstMpegtsMiscDescriptorType">
      <doc xml:space="preserve">The type of #GstMpegtsDescriptor

These values correspond to miscellaneous descriptor types that are
not yet identified from known specifications.</doc>
      
      <member name="ac3_audio_stream" value="129" c:identifier="GST_MTS_DESC_AC3_AUDIO_STREAM">
      </member>
      <member name="dtg_logical_channel" value="131" c:identifier="GST_MTS_DESC_DTG_LOGICAL_CHANNEL">
      </member>
    </enumeration>
    <enumeration name="ModulationType" c:type="GstMpegtsModulationType">
      
      <member name="qpsk" value="0" c:identifier="GST_MPEGTS_MODULATION_QPSK">
      </member>
      <member name="qam_16" value="1" c:identifier="GST_MPEGTS_MODULATION_QAM_16">
      </member>
      <member name="qam_32" value="2" c:identifier="GST_MPEGTS_MODULATION_QAM_32">
      </member>
      <member name="qam_64" value="3" c:identifier="GST_MPEGTS_MODULATION_QAM_64">
      </member>
      <member name="qam_128" value="4" c:identifier="GST_MPEGTS_MODULATION_QAM_128">
      </member>
      <member name="qam_256" value="5" c:identifier="GST_MPEGTS_MODULATION_QAM_256">
      </member>
      <member name="qam_auto" value="6" c:identifier="GST_MPEGTS_MODULATION_QAM_AUTO">
      </member>
      <member name="vsb_8" value="7" c:identifier="GST_MPEGTS_MODULATION_VSB_8">
      </member>
      <member name="vsb_16" value="8" c:identifier="GST_MPEGTS_MODULATION_VSB_16">
      </member>
      <member name="psk_8" value="9" c:identifier="GST_MPEGTS_MODULATION_PSK_8">
      </member>
      <member name="apsk_16" value="10" c:identifier="GST_MPEGTS_MODULATION_APSK_16">
      </member>
      <member name="apsk_32" value="11" c:identifier="GST_MPEGTS_MODULATION_APSK_32">
      </member>
      <member name="dqpsk" value="12" c:identifier="GST_MPEGTS_MODULATION_DQPSK">
      </member>
      <member name="qam_4_nr_" value="13" c:identifier="GST_MPEGTS_MODULATION_QAM_4_NR_">
      </member>
      <member name="none" value="14" c:identifier="GST_MPEGTS_MODULATION_NONE">
      </member>
    </enumeration>
    <record name="NIT" c:type="GstMpegtsNIT" glib:type-name="GstMpegtsNIT" glib:get-type="gst_mpegts_nit_get_type" c:symbol-prefix="nit">
      <doc xml:space="preserve">Network Information Table (ISO/IEC 13818-1 / EN 300 468)</doc>
      
      <field name="actual_network" writable="1">
        <doc xml:space="preserve">Whether this NIT corresponds to the actual stream</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="network_id" writable="1">
        <doc xml:space="preserve">ID of the network that this NIT describes</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">the global descriptors</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
      <field name="streams" writable="1">
        <doc xml:space="preserve">the streams</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="NITStream"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_nit_new">
        <doc xml:space="preserve">Allocates and initializes a #GstMpegtsNIT.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">A newly allocated #GstMpegtsNIT</doc>
          <type name="NIT" c:type="GstMpegtsNIT*"/>
        </return-value>
      </constructor>
    </record>
    <record name="NITStream" c:type="GstMpegtsNITStream" glib:type-name="GstMpegtsNITStream" glib:get-type="gst_mpegts_nit_stream_get_type" c:symbol-prefix="nit_stream">
      
      <field name="transport_stream_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="original_network_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="descriptors" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_nit_stream_new">
        <doc xml:space="preserve">Allocates and initializes a #GstMpegtsNITStream</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">A newly allocated #GstMpegtsNITStream</doc>
          <type name="NITStream" c:type="GstMpegtsNITStream*"/>
        </return-value>
      </constructor>
    </record>
    <record name="PMT" c:type="GstMpegtsPMT" glib:type-name="GstMpegtsPMT" glib:get-type="gst_mpegts_pmt_get_type" c:symbol-prefix="pmt">
      <doc xml:space="preserve">Program Map Table (ISO/IEC 13818-1).

The program_number is contained in the subtable_extension field of the
container #GstMpegtsSection.</doc>
      
      <field name="pcr_pid" writable="1">
        <doc xml:space="preserve">PID of the stream containing PCR</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="program_number" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">array of #GstMpegtsDescriptor</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
      <field name="streams" writable="1">
        <doc xml:space="preserve">Array of #GstMpegtsPMTStream</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="PMTStream"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_pmt_new">
        <doc xml:space="preserve">Allocates and initializes a new #GstMpegtsPMT.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">#GstMpegtsPMT</doc>
          <type name="PMT" c:type="GstMpegtsPMT*"/>
        </return-value>
      </constructor>
    </record>
    <record name="PMTStream" c:type="GstMpegtsPMTStream" glib:type-name="GstMpegtsPMTStream" glib:get-type="gst_mpegts_pmt_stream_get_type" c:symbol-prefix="pmt_stream">
      <doc xml:space="preserve">An individual stream definition.</doc>
      
      <field name="stream_type" writable="1">
        <doc xml:space="preserve">the type of stream. See #GstMpegtsStreamType</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="pid" writable="1">
        <doc xml:space="preserve">the PID of the stream</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">the descriptors of the
stream</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_pmt_stream_new">
        <doc xml:space="preserve">Allocates and initializes a new #GstMpegtsPMTStream.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">#GstMpegtsPMTStream</doc>
          <type name="PMTStream" c:type="GstMpegtsPMTStream*"/>
        </return-value>
      </constructor>
    </record>
    <callback name="PacketizeFunc" c:type="GstMpegtsPacketizeFunc">
      
      <return-value transfer-ownership="none">
        <type name="gboolean" c:type="gboolean"/>
      </return-value>
      <parameters>
        <parameter name="section" transfer-ownership="none">
          <type name="Section" c:type="GstMpegtsSection*"/>
        </parameter>
      </parameters>
    </callback>
    <record name="PatProgram" c:type="GstMpegtsPatProgram" glib:type-name="GstMpegtsPatProgram" glib:get-type="gst_mpegts_pat_program_get_type" c:symbol-prefix="pat_program">
      <doc xml:space="preserve">A program entry from a Program Association Table (ITU H.222.0, ISO/IEC 13818-1).</doc>
      
      <field name="program_number" writable="1">
        <doc xml:space="preserve">the program number</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="network_or_program_map_PID" writable="1">
        <doc xml:space="preserve">the network of program map PID</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_pat_program_new">
        <doc xml:space="preserve">Allocates a new #GstMpegtsPatProgram.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">A newly allocated #GstMpegtsPatProgram</doc>
          <type name="PatProgram" c:type="GstMpegtsPatProgram*"/>
        </return-value>
      </constructor>
    </record>
    <enumeration name="RunningStatus" c:type="GstMpegtsRunningStatus">
      <doc xml:space="preserve">Running status of a service.

Corresponds to table 6 of ETSI EN 300 468 (v1.13.0)</doc>
      
      <member name="undefined" value="0" c:identifier="GST_MPEGTS_RUNNING_STATUS_UNDEFINED">
      </member>
      <member name="not_running" value="1" c:identifier="GST_MPEGTS_RUNNING_STATUS_NOT_RUNNING">
      </member>
      <member name="starts_in_few_seconds" value="2" c:identifier="GST_MPEGTS_RUNNING_STATUS_STARTS_IN_FEW_SECONDS">
      </member>
      <member name="pausing" value="3" c:identifier="GST_MPEGTS_RUNNING_STATUS_PAUSING">
      </member>
      <member name="running" value="4" c:identifier="GST_MPEGTS_RUNNING_STATUS_RUNNING">
      </member>
      <member name="off_air" value="5" c:identifier="GST_MPEGTS_RUNNING_STATUS_OFF_AIR">
      </member>
    </enumeration>
    <record name="SCTESIT" c:type="GstMpegtsSCTESIT" glib:type-name="GstMpegtsSCTESIT" glib:get-type="gst_mpegts_scte_sit_get_type" c:symbol-prefix="scte_sit">
      
      <field name="encrypted_packet" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="encryption_algorithm" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="pts_adjustment" writable="1">
        <type name="guint64" c:type="guint64"/>
      </field>
      <field name="cw_index" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="tier" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="splice_command_length" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="splice_command_type" writable="1">
        <type name="SCTESpliceCommandType" c:type="GstMpegtsSCTESpliceCommandType"/>
      </field>
      <field name="splice_time_specified" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="splice_time" writable="1">
        <type name="guint64" c:type="guint64"/>
      </field>
      <field name="splices" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="gpointer" c:type="gpointer"/>
        </array>
      </field>
      <field name="descriptors" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="gpointer" c:type="gpointer"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_scte_sit_new">
        <doc xml:space="preserve">Allocates and initializes a #GstMpegtsSCTESIT.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">A newly allocated #GstMpegtsSCTESIT</doc>
          <type name="SCTESIT" c:type="GstMpegtsSCTESIT*"/>
        </return-value>
      </constructor>
    </record>
    <enumeration name="SCTESpliceCommandType" c:type="GstMpegtsSCTESpliceCommandType">
      
      <member name="null" value="0" c:identifier="GST_MTS_SCTE_SPLICE_COMMAND_NULL">
      </member>
      <member name="schedule" value="4" c:identifier="GST_MTS_SCTE_SPLICE_COMMAND_SCHEDULE">
      </member>
      <member name="insert" value="5" c:identifier="GST_MTS_SCTE_SPLICE_COMMAND_INSERT">
      </member>
      <member name="time" value="6" c:identifier="GST_MTS_SCTE_SPLICE_COMMAND_TIME">
      </member>
      <member name="bandwidth" value="7" c:identifier="GST_MTS_SCTE_SPLICE_COMMAND_BANDWIDTH">
      </member>
      <member name="private" value="255" c:identifier="GST_MTS_SCTE_SPLICE_COMMAND_PRIVATE">
      </member>
    </enumeration>
    <enumeration name="SCTESpliceDescriptor" c:type="GstMpegtsSCTESpliceDescriptor">
      
      <member name="avail" value="0" c:identifier="GST_MTS_SCTE_DESC_AVAIL">
      </member>
      <member name="dtmf" value="1" c:identifier="GST_MTS_SCTE_DESC_DTMF">
      </member>
      <member name="segmentation" value="2" c:identifier="GST_MTS_SCTE_DESC_SEGMENTATION">
      </member>
      <member name="time" value="3" c:identifier="GST_MTS_SCTE_DESC_TIME">
      </member>
      <member name="audio" value="4" c:identifier="GST_MTS_SCTE_DESC_AUDIO">
      </member>
    </enumeration>
    <record name="SCTESpliceEvent" c:type="GstMpegtsSCTESpliceEvent" glib:type-name="GstMpegtsSCTESpliceEvent" glib:get-type="gst_mpegts_scte_splice_event_get_type" c:symbol-prefix="scte_splice_event">
      
      <field name="insert_event" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="splice_event_id" writable="1">
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="splice_event_cancel_indicator" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="out_of_network_indicator" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="program_splice_flag" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="duration_flag" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="splice_immediate_flag" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="program_splice_time_specified" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="program_splice_time" writable="1">
        <type name="guint64" c:type="guint64"/>
      </field>
      <field name="break_duration_auto_return" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="break_duration" writable="1">
        <type name="guint64" c:type="guint64"/>
      </field>
      <field name="unique_program_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="avail_num" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="avails_expected" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_scte_splice_event_new">
        <doc xml:space="preserve">Allocates and initializes a #GstMpegtsSCTESpliceEvent.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">A newly allocated #GstMpegtsSCTESpliceEvent</doc>
          <type name="SCTESpliceEvent" c:type="GstMpegtsSCTESpliceEvent*"/>
        </return-value>
      </constructor>
    </record>
    <record name="SDT" c:type="GstMpegtsSDT" glib:type-name="GstMpegtsSDT" glib:get-type="gst_mpegts_sdt_get_type" c:symbol-prefix="sdt">
      <doc xml:space="preserve">Service Description Table (EN 300 468)</doc>
      
      <field name="original_network_id" writable="1">
        <doc xml:space="preserve">Network ID of the originating delivery system</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="actual_ts" writable="1">
        <doc xml:space="preserve">True if the table describes this transport stream</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="transport_stream_id" writable="1">
        <doc xml:space="preserve">ID of this transport stream</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="services" writable="1">
        <doc xml:space="preserve">List of services</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="SDTService"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_sdt_new">
        <doc xml:space="preserve">Allocates and initializes a #GstMpegtsSDT.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">A newly allocated #GstMpegtsSDT</doc>
          <type name="SDT" c:type="GstMpegtsSDT*"/>
        </return-value>
      </constructor>
    </record>
    <record name="SDTService" c:type="GstMpegtsSDTService" glib:type-name="GstMpegtsSDTService" glib:get-type="gst_mpegts_sdt_service_get_type" c:symbol-prefix="sdt_service">
      
      <field name="service_id" writable="1">
        <doc xml:space="preserve">The program number this table belongs to</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="EIT_schedule_flag" writable="1">
        <doc xml:space="preserve">EIT schedule information is present in this transport stream</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="EIT_present_following_flag" writable="1">
        <doc xml:space="preserve">EIT present/following information is present in this transport stream</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="running_status" writable="1">
        <doc xml:space="preserve">Status of this service</doc>
        <type name="RunningStatus" c:type="GstMpegtsRunningStatus"/>
      </field>
      <field name="free_CA_mode" writable="1">
        <doc xml:space="preserve">True if one or more streams is controlled by a CA system</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">List of descriptors</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_sdt_service_new">
        <doc xml:space="preserve">Allocates and initializes a #GstMpegtsSDTService.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">A newly allocated #GstMpegtsSDTService</doc>
          <type name="SDTService" c:type="GstMpegtsSDTService*"/>
        </return-value>
      </constructor>
    </record>
    <function-macro name="SECTION" c:identifier="GST_MPEGTS_SECTION" introspectable="0">
      
      <parameters>
        <parameter name="section">
        </parameter>
      </parameters>
    </function-macro>
    <function-macro name="SECTION_TYPE" c:identifier="GST_MPEGTS_SECTION_TYPE" introspectable="0">
      
      <parameters>
        <parameter name="section">
        </parameter>
      </parameters>
    </function-macro>
    <record name="SatelliteDeliverySystemDescriptor" c:type="GstMpegtsSatelliteDeliverySystemDescriptor" glib:type-name="GstMpegtsSatelliteDeliverySystemDescriptor" glib:get-type="gst_mpegts_satellite_delivery_system_descriptor_get_type" c:symbol-prefix="satellite_delivery_system_descriptor">
      <doc xml:space="preserve">Satellite Delivery System Descriptor (EN 300 468 v.1.13.1)</doc>
      
      <field name="frequency" writable="1">
        <doc xml:space="preserve">the frequency in kHz (kiloHertz)</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="orbital_position" writable="1">
        <doc xml:space="preserve">the orbital position in degrees</doc>
        <type name="gfloat" c:type="gfloat"/>
      </field>
      <field name="west_east" writable="1">
        <doc xml:space="preserve">If %TRUE, the satellite is in the eastern part of the orbit,
else in the western part.</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="polarization" writable="1">
        <doc xml:space="preserve">The polarization of the transmitted signal</doc>
        <type name="SatellitePolarizationType" c:type="GstMpegtsSatellitePolarizationType"/>
      </field>
      <field name="roll_off" writable="1">
        <doc xml:space="preserve">Roll-off factor used in DVB-S2</doc>
        <type name="SatelliteRolloff" c:type="GstMpegtsSatelliteRolloff"/>
      </field>
      <field name="modulation_system" writable="1">
        <doc xml:space="preserve">modulation system, %TRUE if DVB-S2, else DVB-S</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="modulation_type" writable="1">
        <doc xml:space="preserve">Modulation scheme used</doc>
        <type name="ModulationType" c:type="GstMpegtsModulationType"/>
      </field>
      <field name="symbol_rate" writable="1">
        <doc xml:space="preserve">Symbol rate (in symbols per second)</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="fec_inner" writable="1">
        <doc xml:space="preserve">inner FEC scheme used</doc>
        <type name="DVBCodeRate" c:type="GstMpegtsDVBCodeRate"/>
      </field>
    </record>
    <enumeration name="SatellitePolarizationType" c:type="GstMpegtsSatellitePolarizationType">
      
      <member name="linear_horizontal" value="0" c:identifier="GST_MPEGTS_POLARIZATION_LINEAR_HORIZONTAL">
      </member>
      <member name="linear_vertical" value="1" c:identifier="GST_MPEGTS_POLARIZATION_LINEAR_VERTICAL">
      </member>
      <member name="circular_left" value="2" c:identifier="GST_MPEGTS_POLARIZATION_CIRCULAR_LEFT">
      </member>
      <member name="circular_right" value="3" c:identifier="GST_MPEGTS_POLARIZATION_CIRCULAR_RIGHT">
      </member>
    </enumeration>
    <enumeration name="SatelliteRolloff" c:type="GstMpegtsSatelliteRolloff">
      
      <member name="35" value="0" c:identifier="GST_MPEGTS_ROLLOFF_35">
      </member>
      <member name="20" value="1" c:identifier="GST_MPEGTS_ROLLOFF_20">
      </member>
      <member name="25" value="2" c:identifier="GST_MPEGTS_ROLLOFF_25">
      </member>
      <member name="reserved" value="3" c:identifier="GST_MPEGTS_ROLLOFF_RESERVED">
      </member>
      <member name="auto" value="4" c:identifier="GST_MPEGTS_ROLLOFF_AUTO">
      </member>
    </enumeration>
    <enumeration name="ScteStreamType" c:type="GstMpegtsScteStreamType">
      <doc xml:space="preserve">Type of mpeg-ts streams for SCTE</doc>
      
      <member name="subtitling" value="130" c:identifier="GST_MPEGTS_STREAM_TYPE_SCTE_SUBTITLING">
        <doc xml:space="preserve">SCTE-27 Subtitling</doc>
      </member>
      <member name="isoch_data" value="131" c:identifier="GST_MPEGTS_STREAM_TYPE_SCTE_ISOCH_DATA">
        <doc xml:space="preserve">SCTE-19 Isochronous data</doc>
      </member>
      <member name="sit" value="134" c:identifier="GST_MPEGTS_STREAM_TYPE_SCTE_SIT">
        <doc xml:space="preserve">SCTE-35 Splice Information Table</doc>
      </member>
      <member name="dst_nrt" value="149" c:identifier="GST_MPEGTS_STREAM_TYPE_SCTE_DST_NRT">
        <doc xml:space="preserve">SCTE-07 Data Service or
Network Resource Table</doc>
      </member>
      <member name="dsmcc_dcb" value="176" c:identifier="GST_MPEGTS_STREAM_TYPE_SCTE_DSMCC_DCB">
        <doc xml:space="preserve">Type B - DSM-CC Data Carousel
[IEC 13818-6])</doc>
      </member>
      <member name="signaling" value="192" c:identifier="GST_MPEGTS_STREAM_TYPE_SCTE_SIGNALING">
        <doc xml:space="preserve">Enhanced Television Application
Signaling (OC-SP-ETV-AM1.0.1-120614)</doc>
      </member>
      <member name="sync_data" value="194" c:identifier="GST_MPEGTS_STREAM_TYPE_SCTE_SYNC_DATA">
        <doc xml:space="preserve">SCTE-07 Synchronous data</doc>
      </member>
      <member name="async_data" value="195" c:identifier="GST_MPEGTS_STREAM_TYPE_SCTE_ASYNC_DATA">
        <doc xml:space="preserve">SCTE-53 Asynchronous data</doc>
      </member>
    </enumeration>
    <record name="Section" c:type="GstMpegtsSection" glib:type-name="GstMpegtsSection" glib:get-type="gst_mpegts_section_get_type" c:symbol-prefix="section">
      <doc xml:space="preserve">For more details, refer to the ITU H.222.0 or ISO/IEC 13818-1 specifications
and other specifications mentioned in the documentation.</doc>
      
      <field name="parent" readable="0" private="1">
        <type name="Gst.MiniObject" c:type="GstMiniObject"/>
      </field>
      <field name="section_type" writable="1">
        <doc xml:space="preserve">The type of section</doc>
        <type name="SectionType" c:type="GstMpegtsSectionType"/>
      </field>
      <field name="pid" writable="1">
        <doc xml:space="preserve">The pid on which this section was found</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="table_id" writable="1">
        <doc xml:space="preserve">The table id of this section</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="subtable_extension" writable="1">
        <doc xml:space="preserve">This meaning differs per section. See the documentation
of the parsed section type for the meaning of this field</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="version_number" writable="1">
        <doc xml:space="preserve">Version of the section.</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="current_next_indicator" writable="1">
        <doc xml:space="preserve">Applies to current/next stream or not</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="section_number" writable="1">
        <doc xml:space="preserve">Number of the section (if multiple)</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="last_section_number" writable="1">
        <doc xml:space="preserve">Number of the last expected section (if multiple)</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="crc" writable="1">
        <doc xml:space="preserve">CRC</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="data" readable="0" private="1">
        <type name="guint8" c:type="guint8*"/>
      </field>
      <field name="section_length" readable="0" private="1">
        <type name="guint" c:type="guint"/>
      </field>
      <field name="cached_parsed" readable="0" private="1">
        <type name="gpointer" c:type="gpointer*"/>
      </field>
      <field name="destroy_parsed" readable="0" private="1">
        <type name="GLib.DestroyNotify" c:type="GDestroyNotify"/>
      </field>
      <field name="offset" readable="0" private="1">
        <type name="guint64" c:type="guint64"/>
      </field>
      <field name="short_section" readable="0" private="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="packetizer" readable="0" private="1">
        <type name="PacketizeFunc" c:type="GstMpegtsPacketizeFunc"/>
      </field>
      <field name="_gst_reserved" readable="0" private="1">
        <array zero-terminated="0" fixed-size="4">
          <type name="gpointer" c:type="gpointer"/>
        </array>
      </field>
      <constructor name="new" c:identifier="gst_mpegts_section_new">
        <doc xml:space="preserve">Creates a new #GstMpegtsSection from the provided @data.

Note: Ensuring @data is big enough to contain the full section is the
responsibility of the caller. If it is not big enough, %NULL will be
returned.

Note: it is the responsibility of the caller to ensure @data does point
to the beginning of the section.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">A new #GstMpegtsSection if the data was valid,
else %NULL</doc>
          <type name="Section" c:type="GstMpegtsSection*"/>
        </return-value>
        <parameters>
          <parameter name="pid" transfer-ownership="none">
            <doc xml:space="preserve">the PID to which this section belongs</doc>
            <type name="guint16" c:type="guint16"/>
          </parameter>
          <parameter name="data" transfer-ownership="full">
            <doc xml:space="preserve">a pointer to the beginning of the section (i.e. the first byte
should contain the table_id field).</doc>
            <array length="2" zero-terminated="0" c:type="guint8*">
              <type name="guint8" c:type="guint8"/>
            </array>
          </parameter>
          <parameter name="data_size" transfer-ownership="none">
            <doc xml:space="preserve">size of the @data argument.</doc>
            <type name="gsize" c:type="gsize"/>
          </parameter>
        </parameters>
      </constructor>
      <method name="get_atsc_cvct" c:identifier="gst_mpegts_section_get_atsc_cvct">
        <doc xml:space="preserve">Returns the #GstMpegtsAtscVCT contained in the @section</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsAtscVCT contained in the section, or %NULL if an error
happened.</doc>
          <type name="AtscVCT" c:type="const GstMpegtsAtscVCT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_ATSC_CVCT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_atsc_eit" c:identifier="gst_mpegts_section_get_atsc_eit">
        <doc xml:space="preserve">Returns the #GstMpegtsAtscEIT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsAtscEIT contained in the section, or %NULL if an error
happened.</doc>
          <type name="AtscEIT" c:type="const GstMpegtsAtscEIT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_ATSC_EIT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_atsc_ett" c:identifier="gst_mpegts_section_get_atsc_ett">
        <doc xml:space="preserve">Returns the #GstMpegtsAtscETT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsAtscETT contained in the section, or %NULL if an error
happened.</doc>
          <type name="AtscETT" c:type="const GstMpegtsAtscETT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_ATSC_ETT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_atsc_mgt" c:identifier="gst_mpegts_section_get_atsc_mgt">
        <doc xml:space="preserve">Returns the #GstMpegtsAtscMGT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsAtscMGT contained in the section, or %NULL if an error
happened.</doc>
          <type name="AtscMGT" c:type="const GstMpegtsAtscMGT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_ATSC_MGT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_atsc_rrt" c:identifier="gst_mpegts_section_get_atsc_rrt" version="1.18">
        <doc xml:space="preserve">Returns the #GstMpegtsAtscRRT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsAtscRRT contained in the section, or %NULL if an error
happened.</doc>
          <type name="AtscRRT" c:type="const GstMpegtsAtscRRT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_ATSC_RRT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_atsc_stt" c:identifier="gst_mpegts_section_get_atsc_stt">
        <doc xml:space="preserve">Returns the #GstMpegtsAtscSTT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsAtscSTT contained in the section, or %NULL if an error
happened.</doc>
          <type name="AtscSTT" c:type="const GstMpegtsAtscSTT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_ATSC_STT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_atsc_tvct" c:identifier="gst_mpegts_section_get_atsc_tvct">
        <doc xml:space="preserve">Returns the #GstMpegtsAtscVCT contained in the @section</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsAtscVCT contained in the section, or %NULL if an error
happened.</doc>
          <type name="AtscVCT" c:type="const GstMpegtsAtscVCT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_ATSC_TVCT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_bat" c:identifier="gst_mpegts_section_get_bat">
        <doc xml:space="preserve">Returns the #GstMpegtsBAT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsBAT contained in the section, or %NULL if an error
happened.</doc>
          <type name="BAT" c:type="const GstMpegtsBAT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_BAT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_cat" c:identifier="gst_mpegts_section_get_cat">
        <doc xml:space="preserve">Returns the array of #GstMpegtsDescriptor contained in the Conditional
Access Table.</doc>
        
        <return-value transfer-ownership="container">
          <doc xml:space="preserve">The
#GstMpegtsDescriptor contained in the section, or %NULL if an error
happened. Release with #g_array_unref when done.</doc>
          <array name="GLib.PtrArray" c:type="GPtrArray*">
            <type name="Descriptor"/>
          </array>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_CAT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_data" c:identifier="gst_mpegts_section_get_data">
        <doc xml:space="preserve">Gets the original unparsed section data.</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">The original unparsed section data.</doc>
          <type name="GLib.Bytes" c:type="GBytes*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_eit" c:identifier="gst_mpegts_section_get_eit">
        <doc xml:space="preserve">Returns the #GstMpegtsEIT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsEIT contained in the section, or %NULL if an error
happened.</doc>
          <type name="EIT" c:type="const GstMpegtsEIT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_EIT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_nit" c:identifier="gst_mpegts_section_get_nit">
        <doc xml:space="preserve">Returns the #GstMpegtsNIT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsNIT contained in the section, or %NULL if an error
happened.</doc>
          <type name="NIT" c:type="const GstMpegtsNIT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_NIT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_pat" c:identifier="gst_mpegts_section_get_pat">
        <doc xml:space="preserve">Parses a Program Association Table (ITU H.222.0, ISO/IEC 13818-1).

Returns the array of #GstMpegtsPatProgram contained in the section.

Note: The PAT "transport_id" field corresponds to the "subtable_extension"
field of the provided @section.</doc>
        
        <return-value transfer-ownership="container">
          <doc xml:space="preserve">The
#GstMpegtsPatProgram contained in the section, or %NULL if an error
happened. Release with #g_ptr_array_unref when done.</doc>
          <array name="GLib.PtrArray" c:type="GPtrArray*">
            <type name="PatProgram"/>
          </array>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_PAT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_pmt" c:identifier="gst_mpegts_section_get_pmt">
        <doc xml:space="preserve">Returns the #GstMpegtsPMT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsPMT contained in the section, or %NULL if an error
happened.</doc>
          <type name="PMT" c:type="const GstMpegtsPMT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_PMT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_scte_sit" c:identifier="gst_mpegts_section_get_scte_sit">
        <doc xml:space="preserve">Returns the #GstMpegtsSCTESIT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsSCTESIT contained in the section, or %NULL if an error
happened.</doc>
          <type name="SCTESIT" c:type="const GstMpegtsSCTESIT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_SCTE_SIT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_sdt" c:identifier="gst_mpegts_section_get_sdt">
        <doc xml:space="preserve">Returns the #GstMpegtsSDT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsSDT contained in the section, or %NULL if an error
happened.</doc>
          <type name="SDT" c:type="const GstMpegtsSDT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_SDT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_tdt" c:identifier="gst_mpegts_section_get_tdt">
        <doc xml:space="preserve">Returns the #GstDateTime of the TDT</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">The #GstDateTime contained in the section, or %NULL
if an error happened. Release with #gst_date_time_unref when done.</doc>
          <type name="Gst.DateTime" c:type="GstDateTime*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_TDT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_tot" c:identifier="gst_mpegts_section_get_tot">
        <doc xml:space="preserve">Returns the #GstMpegtsTOT contained in the @section.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsTOT contained in the section, or %NULL if an error
happened.</doc>
          <type name="TOT" c:type="const GstMpegtsTOT*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_TOT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="get_tsdt" c:identifier="gst_mpegts_section_get_tsdt">
        <doc xml:space="preserve">Returns the array of #GstMpegtsDescriptor contained in the section</doc>
        
        <return-value transfer-ownership="container">
          <doc xml:space="preserve">The
#GstMpegtsDescriptor contained in the section, or %NULL if an error
happened. Release with #g_array_unref when done.</doc>
          <array name="GLib.PtrArray" c:type="GPtrArray*">
            <type name="Descriptor"/>
          </array>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">a #GstMpegtsSection of type %GST_MPEGTS_SECTION_TSDT</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
        </parameters>
      </method>
      <method name="packetize" c:identifier="gst_mpegts_section_packetize">
        <doc xml:space="preserve">If the data in @section has already been packetized, the data pointer is returned
immediately. Otherwise, the data field is allocated and populated.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">pointer to section data, or %NULL on fail</doc>
          <type name="guint8" c:type="guint8*"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">the #GstMpegtsSection that holds the data</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
          <parameter name="output_size" direction="out" caller-allocates="0" transfer-ownership="full">
            <doc xml:space="preserve">#gsize to hold the size of the data</doc>
            <type name="gsize" c:type="gsize*"/>
          </parameter>
        </parameters>
      </method>
      <method name="send_event" c:identifier="gst_mpegts_section_send_event">
        <doc xml:space="preserve">Creates a custom #GstEvent with a @GstMpegtsSection.
The #GstEvent is sent to the @element #GstElement.</doc>
        
        <return-value transfer-ownership="none">
          <doc xml:space="preserve">%TRUE if the event is sent</doc>
          <type name="gboolean" c:type="gboolean"/>
        </return-value>
        <parameters>
          <instance-parameter name="section" transfer-ownership="none">
            <doc xml:space="preserve">The #GstMpegtsSection to put in the event</doc>
            <type name="Section" c:type="GstMpegtsSection*"/>
          </instance-parameter>
          <parameter name="element" transfer-ownership="none">
            <doc xml:space="preserve">The #GstElement to send to section event to</doc>
            <type name="Gst.Element" c:type="GstElement*"/>
          </parameter>
        </parameters>
      </method>
      <function name="from_atsc_mgt" c:identifier="gst_mpegts_section_from_atsc_mgt" version="1.18">
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">the #GstMpegtsSection</doc>
          <type name="Section" c:type="GstMpegtsSection*"/>
        </return-value>
        <parameters>
          <parameter name="mgt" transfer-ownership="full">
            <doc xml:space="preserve">a #GstMpegtsAtscMGT to create the #GstMpegtsSection from</doc>
            <type name="AtscMGT" c:type="GstMpegtsAtscMGT*"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_atsc_rrt" c:identifier="gst_mpegts_section_from_atsc_rrt">
        
        <return-value transfer-ownership="full">
          <type name="Section" c:type="GstMpegtsSection*"/>
        </return-value>
        <parameters>
          <parameter name="rrt" transfer-ownership="none">
            <type name="AtscRRT" c:type="GstMpegtsAtscRRT*"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_atsc_stt" c:identifier="gst_mpegts_section_from_atsc_stt">
        
        <return-value transfer-ownership="full">
          <type name="Section" c:type="GstMpegtsSection*"/>
        </return-value>
        <parameters>
          <parameter name="stt" transfer-ownership="none">
            <type name="AtscSTT" c:type="GstMpegtsAtscSTT*"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_nit" c:identifier="gst_mpegts_section_from_nit">
        <doc xml:space="preserve">Ownership of @nit is taken. The data in @nit is managed by the #GstMpegtsSection</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">the #GstMpegtsSection</doc>
          <type name="Section" c:type="GstMpegtsSection*"/>
        </return-value>
        <parameters>
          <parameter name="nit" transfer-ownership="full">
            <doc xml:space="preserve">a #GstMpegtsNIT to create the #GstMpegtsSection from</doc>
            <type name="NIT" c:type="GstMpegtsNIT*"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_pat" c:identifier="gst_mpegts_section_from_pat">
        <doc xml:space="preserve">Creates a PAT #GstMpegtsSection from the @programs array of #GstMpegtsPatPrograms</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">a #GstMpegtsSection</doc>
          <type name="Section" c:type="GstMpegtsSection*"/>
        </return-value>
        <parameters>
          <parameter name="programs" transfer-ownership="full">
            <doc xml:space="preserve">an array of #GstMpegtsPatProgram</doc>
            <array name="GLib.PtrArray" c:type="GPtrArray*">
              <type name="PatProgram"/>
            </array>
          </parameter>
          <parameter name="ts_id" transfer-ownership="none">
            <doc xml:space="preserve">Transport stream ID of the PAT</doc>
            <type name="guint16" c:type="guint16"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_pmt" c:identifier="gst_mpegts_section_from_pmt">
        <doc xml:space="preserve">Creates a #GstMpegtsSection from @pmt that is bound to @pid</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">#GstMpegtsSection</doc>
          <type name="Section" c:type="GstMpegtsSection*"/>
        </return-value>
        <parameters>
          <parameter name="pmt" transfer-ownership="full">
            <doc xml:space="preserve">a #GstMpegtsPMT to create a #GstMpegtsSection from</doc>
            <type name="PMT" c:type="GstMpegtsPMT*"/>
          </parameter>
          <parameter name="pid" transfer-ownership="none">
            <doc xml:space="preserve">The PID that the #GstMpegtsPMT belongs to</doc>
            <type name="guint16" c:type="guint16"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_scte_sit" c:identifier="gst_mpegts_section_from_scte_sit">
        <doc xml:space="preserve">Ownership of @sit is taken. The data in @sit is managed by the #GstMpegtsSection</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">the #GstMpegtsSection</doc>
          <type name="Section" c:type="GstMpegtsSection*"/>
        </return-value>
        <parameters>
          <parameter name="sit" transfer-ownership="full">
            <doc xml:space="preserve">a #GstMpegtsSCTESIT to create the #GstMpegtsSection from</doc>
            <type name="SCTESIT" c:type="GstMpegtsSCTESIT*"/>
          </parameter>
          <parameter name="pid" transfer-ownership="none">
            <type name="guint16" c:type="guint16"/>
          </parameter>
        </parameters>
      </function>
      <function name="from_sdt" c:identifier="gst_mpegts_section_from_sdt">
        <doc xml:space="preserve">Ownership of @sdt is taken. The data in @sdt is managed by the #GstMpegtsSection</doc>
        
        <return-value transfer-ownership="full">
          <doc xml:space="preserve">the #GstMpegtsSection</doc>
          <type name="Section" c:type="GstMpegtsSection*"/>
        </return-value>
        <parameters>
          <parameter name="sdt" transfer-ownership="full">
            <doc xml:space="preserve">a #GstMpegtsSDT to create the #GstMpegtsSection from</doc>
            <type name="SDT" c:type="GstMpegtsSDT*"/>
          </parameter>
        </parameters>
      </function>
    </record>
    <enumeration name="SectionATSCTableID" c:type="GstMpegtsSectionATSCTableID">
      <doc xml:space="preserve">Values for a #GstMpegtsSection table_id.

These are the registered ATSC table_id variants.

see also: #GstMpegtsSectionTableID</doc>
      
      <member name="master_guide" value="199" c:identifier="GST_MTS_TABLE_ID_ATSC_MASTER_GUIDE">
      </member>
      <member name="terrestrial_virtual_channel" value="200" c:identifier="GST_MTS_TABLE_ID_ATSC_TERRESTRIAL_VIRTUAL_CHANNEL">
      </member>
      <member name="cable_virtual_channel" value="201" c:identifier="GST_MTS_TABLE_ID_ATSC_CABLE_VIRTUAL_CHANNEL">
      </member>
      <member name="rating_region" value="202" c:identifier="GST_MTS_TABLE_ID_ATSC_RATING_REGION">
      </member>
      <member name="event_information" value="203" c:identifier="GST_MTS_TABLE_ID_ATSC_EVENT_INFORMATION">
      </member>
      <member name="channel_or_event_extended_text" value="204" c:identifier="GST_MTS_TABLE_ID_ATSC_CHANNEL_OR_EVENT_EXTENDED_TEXT">
      </member>
      <member name="system_time" value="205" c:identifier="GST_MTS_TABLE_ID_ATSC_SYSTEM_TIME">
      </member>
      <member name="data_event" value="206" c:identifier="GST_MTS_TABLE_ID_ATSC_DATA_EVENT">
      </member>
      <member name="data_service" value="207" c:identifier="GST_MTS_TABLE_ID_ATSC_DATA_SERVICE">
      </member>
      <member name="network_resource" value="209" c:identifier="GST_MTS_TABLE_ID_ATSC_NETWORK_RESOURCE">
      </member>
      <member name="long_term_service" value="210" c:identifier="GST_MTS_TABLE_ID_ATSC_LONG_TERM_SERVICE">
      </member>
      <member name="directed_channel_change" value="211" c:identifier="GST_MTS_TABLE_ID_ATSC_DIRECTED_CHANNEL_CHANGE">
      </member>
      <member name="directed_channel_change_section_code" value="212" c:identifier="GST_MTS_TABLE_ID_ATSC_DIRECTED_CHANNEL_CHANGE_SECTION_CODE">
      </member>
      <member name="aggregate_event_information" value="214" c:identifier="GST_MTS_TABLE_ID_ATSC_AGGREGATE_EVENT_INFORMATION">
      </member>
      <member name="aggregate_extended_text" value="215" c:identifier="GST_MTS_TABLE_ID_ATSC_AGGREGATE_EXTENDED_TEXT">
      </member>
      <member name="aggregate_data_event" value="217" c:identifier="GST_MTS_TABLE_ID_ATSC_AGGREGATE_DATA_EVENT">
      </member>
      <member name="satellite_virtual_channel" value="218" c:identifier="GST_MTS_TABLE_ID_ATSC_SATELLITE_VIRTUAL_CHANNEL">
      </member>
    </enumeration>
    <enumeration name="SectionDVBTableID" c:type="GstMpegtsSectionDVBTableID">
      <doc xml:space="preserve">Values for a #GstMpegtsSection table_id.

These are the registered DVB table_id variants.

see also: #GstMpegtsSectionTableID</doc>
      
      <member name="network_information_actual_network" value="64" c:identifier="GST_MTS_TABLE_ID_NETWORK_INFORMATION_ACTUAL_NETWORK">
      </member>
      <member name="network_information_other_network" value="65" c:identifier="GST_MTS_TABLE_ID_NETWORK_INFORMATION_OTHER_NETWORK">
      </member>
      <member name="service_description_actual_ts" value="66" c:identifier="GST_MTS_TABLE_ID_SERVICE_DESCRIPTION_ACTUAL_TS">
      </member>
      <member name="service_description_other_ts" value="70" c:identifier="GST_MTS_TABLE_ID_SERVICE_DESCRIPTION_OTHER_TS">
      </member>
      <member name="bouquet_association" value="74" c:identifier="GST_MTS_TABLE_ID_BOUQUET_ASSOCIATION">
      </member>
      <member name="event_information_actual_ts_present" value="78" c:identifier="GST_MTS_TABLE_ID_EVENT_INFORMATION_ACTUAL_TS_PRESENT">
      </member>
      <member name="event_information_other_ts_present" value="79" c:identifier="GST_MTS_TABLE_ID_EVENT_INFORMATION_OTHER_TS_PRESENT">
      </member>
      <member name="event_information_actual_ts_schedule_1" value="80" c:identifier="GST_MTS_TABLE_ID_EVENT_INFORMATION_ACTUAL_TS_SCHEDULE_1">
      </member>
      <member name="event_information_actual_ts_schedule_n" value="95" c:identifier="GST_MTS_TABLE_ID_EVENT_INFORMATION_ACTUAL_TS_SCHEDULE_N">
      </member>
      <member name="event_information_other_ts_schedule_1" value="96" c:identifier="GST_MTS_TABLE_ID_EVENT_INFORMATION_OTHER_TS_SCHEDULE_1">
      </member>
      <member name="event_information_other_ts_schedule_n" value="111" c:identifier="GST_MTS_TABLE_ID_EVENT_INFORMATION_OTHER_TS_SCHEDULE_N">
      </member>
      <member name="time_date" value="112" c:identifier="GST_MTS_TABLE_ID_TIME_DATE">
      </member>
      <member name="running_status" value="113" c:identifier="GST_MTS_TABLE_ID_RUNNING_STATUS">
      </member>
      <member name="stuffing" value="114" c:identifier="GST_MTS_TABLE_ID_STUFFING">
      </member>
      <member name="time_offset" value="115" c:identifier="GST_MTS_TABLE_ID_TIME_OFFSET">
      </member>
      <member name="application_information_table" value="116" c:identifier="GST_MTS_TABLE_ID_APPLICATION_INFORMATION_TABLE">
      </member>
      <member name="container" value="117" c:identifier="GST_MTS_TABLE_ID_CONTAINER">
      </member>
      <member name="related_content" value="118" c:identifier="GST_MTS_TABLE_ID_RELATED_CONTENT">
      </member>
      <member name="content_identifier" value="119" c:identifier="GST_MTS_TABLE_ID_CONTENT_IDENTIFIER">
      </member>
      <member name="mpe_fec" value="120" c:identifier="GST_MTS_TABLE_ID_MPE_FEC">
      </member>
      <member name="resolution_notification" value="121" c:identifier="GST_MTS_TABLE_ID_RESOLUTION_NOTIFICATION">
      </member>
      <member name="mpe_ifec" value="122" c:identifier="GST_MTS_TABLE_ID_MPE_IFEC">
      </member>
      <member name="discontinuity_information" value="126" c:identifier="GST_MTS_TABLE_ID_DISCONTINUITY_INFORMATION">
      </member>
      <member name="selection_information" value="127" c:identifier="GST_MTS_TABLE_ID_SELECTION_INFORMATION">
      </member>
      <member name="ca_message_ecm_0" value="128" c:identifier="GST_MTS_TABLE_ID_CA_MESSAGE_ECM_0">
      </member>
      <member name="ca_message_ecm_1" value="129" c:identifier="GST_MTS_TABLE_ID_CA_MESSAGE_ECM_1">
      </member>
      <member name="ca_message_system_private_1" value="130" c:identifier="GST_MTS_TABLE_ID_CA_MESSAGE_SYSTEM_PRIVATE_1">
      </member>
      <member name="ca_message_system_private_n" value="143" c:identifier="GST_MTS_TABLE_ID_CA_MESSAGE_SYSTEM_PRIVATE_N">
      </member>
      <member name="sct" value="160" c:identifier="GST_MTS_TABLE_ID_SCT">
      </member>
      <member name="fct" value="161" c:identifier="GST_MTS_TABLE_ID_FCT">
      </member>
      <member name="tct" value="162" c:identifier="GST_MTS_TABLE_ID_TCT">
      </member>
      <member name="spt" value="163" c:identifier="GST_MTS_TABLE_ID_SPT">
      </member>
      <member name="cmt" value="164" c:identifier="GST_MTS_TABLE_ID_CMT">
      </member>
      <member name="tbtp" value="165" c:identifier="GST_MTS_TABLE_ID_TBTP">
      </member>
      <member name="pcr_packet_payload" value="166" c:identifier="GST_MTS_TABLE_ID_PCR_PACKET_PAYLOAD">
      </member>
      <member name="transmission_mode_support_payload" value="170" c:identifier="GST_MTS_TABLE_ID_TRANSMISSION_MODE_SUPPORT_PAYLOAD">
      </member>
      <member name="tim" value="176" c:identifier="GST_MTS_TABLE_ID_TIM">
      </member>
      <member name="ll_fec_parity_data_table" value="177" c:identifier="GST_MTS_TABLE_ID_LL_FEC_PARITY_DATA_TABLE">
      </member>
    </enumeration>
    <enumeration name="SectionSCTETableID" c:type="GstMpegtsSectionSCTETableID">
      <doc xml:space="preserve">Values for a #GstMpegtsSection table_id.

These are the registered SCTE table_id variants.

see also: #GstMpegtsSectionTableID</doc>
      
      <member name="eas" value="216" c:identifier="GST_MTS_TABLE_ID_SCTE_EAS">
        <doc xml:space="preserve">SCTE-18 Emergency Alert System</doc>
      </member>
      <member name="ebif" value="224" c:identifier="GST_MTS_TABLE_ID_SCTE_EBIF">
        <doc xml:space="preserve">CL-SP-ETV-AM 1.0.1 EBIF message</doc>
      </member>
      <member name="reserved" value="225" c:identifier="GST_MTS_TABLE_ID_SCTE_RESERVED">
      </member>
      <member name="eiss" value="226" c:identifier="GST_MTS_TABLE_ID_SCTE_EISS">
        <doc xml:space="preserve">CL-SP-ETV-AM 1.0.1 EBIF Int. Signaling Sect.</doc>
      </member>
      <member name="dii" value="227" c:identifier="GST_MTS_TABLE_ID_SCTE_DII">
        <doc xml:space="preserve">CL-SP-ETV-AM 1.0.1 DSMCC DII message</doc>
      </member>
      <member name="ddb" value="228" c:identifier="GST_MTS_TABLE_ID_SCTE_DDB">
        <doc xml:space="preserve">CL-SP-ETV-AM 1.0.1 DSMCC Data Download Block</doc>
      </member>
      <member name="splice" value="252" c:identifier="GST_MTS_TABLE_ID_SCTE_SPLICE">
        <doc xml:space="preserve">SCTE-35 splice information is carried in a
section stream on a separate PID in the program&#x2019;s Map Table (PMT) allowing
Splice Event notifications to remain associated with the program and pass
through multiplexers.</doc>
      </member>
    </enumeration>
    <enumeration name="SectionTableID" c:type="GstMpegtsSectionTableID">
      <doc xml:space="preserve">Values for a #GstMpegtsSection table_id

These are the registered ITU H.222.0 | ISO/IEC 13818-1 table_id variants.

see also #GstMpegtsSectionATSCTableID, #GstMpegtsSectionDVBTableID, and
#GstMpegtsSectionSCTETableID</doc>
      
      <member name="program_association" value="0" c:identifier="GST_MTS_TABLE_ID_PROGRAM_ASSOCIATION">
      </member>
      <member name="conditional_access" value="1" c:identifier="GST_MTS_TABLE_ID_CONDITIONAL_ACCESS">
      </member>
      <member name="ts_program_map" value="2" c:identifier="GST_MTS_TABLE_ID_TS_PROGRAM_MAP">
      </member>
      <member name="ts_description" value="3" c:identifier="GST_MTS_TABLE_ID_TS_DESCRIPTION">
      </member>
      <member name="14496_scene_description" value="4" c:identifier="GST_MTS_TABLE_ID_14496_SCENE_DESCRIPTION">
      </member>
      <member name="14496_objet_descriptor" value="5" c:identifier="GST_MTS_TABLE_ID_14496_OBJET_DESCRIPTOR">
      </member>
      <member name="metadata" value="6" c:identifier="GST_MTS_TABLE_ID_METADATA">
      </member>
      <member name="ipmp_control_information" value="7" c:identifier="GST_MTS_TABLE_ID_IPMP_CONTROL_INFORMATION">
      </member>
      <member name="dsm_cc_multiproto_encapsulated_data" value="58" c:identifier="GST_MTS_TABLE_ID_DSM_CC_MULTIPROTO_ENCAPSULATED_DATA">
      </member>
      <member name="dsm_cc_u_n_messages" value="59" c:identifier="GST_MTS_TABLE_ID_DSM_CC_U_N_MESSAGES">
      </member>
      <member name="dsm_cc_download_data_messages" value="60" c:identifier="GST_MTS_TABLE_ID_DSM_CC_DOWNLOAD_DATA_MESSAGES">
      </member>
      <member name="dsm_cc_stream_descriptors" value="61" c:identifier="GST_MTS_TABLE_ID_DSM_CC_STREAM_DESCRIPTORS">
      </member>
      <member name="dsm_cc_private_data" value="62" c:identifier="GST_MTS_TABLE_ID_DSM_CC_PRIVATE_DATA">
      </member>
      <member name="dsm_cc_addressable_sections" value="63" c:identifier="GST_MTS_TABLE_ID_DSM_CC_ADDRESSABLE_SECTIONS">
      </member>
      <member name="unset" value="255" c:identifier="GST_MTS_TABLE_ID_UNSET">
      </member>
    </enumeration>
    <enumeration name="SectionType" c:type="GstMpegtsSectionType">
      <doc xml:space="preserve">Types of #GstMpegtsSection that the library handles.</doc>
      
      <member name="unknown" value="0" c:identifier="GST_MPEGTS_SECTION_UNKNOWN">
        <doc xml:space="preserve">Unknown section type</doc>
      </member>
      <member name="pat" value="1" c:identifier="GST_MPEGTS_SECTION_PAT">
        <doc xml:space="preserve">Program Association Table (ISO/IEC 13818-1)</doc>
      </member>
      <member name="pmt" value="2" c:identifier="GST_MPEGTS_SECTION_PMT">
        <doc xml:space="preserve">Program Map Table (ISO/IEC 13818-1)</doc>
      </member>
      <member name="cat" value="3" c:identifier="GST_MPEGTS_SECTION_CAT">
        <doc xml:space="preserve">Conditional Access Table (ISO/IEC 13818-1)</doc>
      </member>
      <member name="tsdt" value="4" c:identifier="GST_MPEGTS_SECTION_TSDT">
        <doc xml:space="preserve">Transport Stream Description Table (ISO/IEC 13818-1)</doc>
      </member>
      <member name="eit" value="5" c:identifier="GST_MPEGTS_SECTION_EIT">
        <doc xml:space="preserve">Event Information Table (EN 300 468)</doc>
      </member>
      <member name="nit" value="6" c:identifier="GST_MPEGTS_SECTION_NIT">
        <doc xml:space="preserve">Network Information Table (ISO/IEC 13818-1 / EN 300 468)</doc>
      </member>
      <member name="bat" value="7" c:identifier="GST_MPEGTS_SECTION_BAT">
        <doc xml:space="preserve">Bouquet Association Table ((EN 300 468)</doc>
      </member>
      <member name="sdt" value="8" c:identifier="GST_MPEGTS_SECTION_SDT">
        <doc xml:space="preserve">Service Description Table (EN 300 468)</doc>
      </member>
      <member name="tdt" value="9" c:identifier="GST_MPEGTS_SECTION_TDT">
        <doc xml:space="preserve">Time and Date Table (EN 300 468)</doc>
      </member>
      <member name="tot" value="10" c:identifier="GST_MPEGTS_SECTION_TOT">
        <doc xml:space="preserve">Time Offset Table (EN 300 468)</doc>
      </member>
      <member name="atsc_tvct" value="11" c:identifier="GST_MPEGTS_SECTION_ATSC_TVCT">
        <doc xml:space="preserve">ATSC Terrestrial Virtual Channel Table (A65)</doc>
      </member>
      <member name="atsc_cvct" value="12" c:identifier="GST_MPEGTS_SECTION_ATSC_CVCT">
        <doc xml:space="preserve">ATSC Cable Virtual Channel Table (A65)</doc>
      </member>
      <member name="atsc_mgt" value="13" c:identifier="GST_MPEGTS_SECTION_ATSC_MGT">
        <doc xml:space="preserve">ATSC Master Guide Table (A65)</doc>
      </member>
      <member name="atsc_ett" value="14" c:identifier="GST_MPEGTS_SECTION_ATSC_ETT">
        <doc xml:space="preserve">ATSC Extended Text Table (A65)</doc>
      </member>
      <member name="atsc_eit" value="15" c:identifier="GST_MPEGTS_SECTION_ATSC_EIT">
        <doc xml:space="preserve">ATSC Event Information Table (A65)</doc>
      </member>
      <member name="atsc_stt" value="16" c:identifier="GST_MPEGTS_SECTION_ATSC_STT">
        <doc xml:space="preserve">ATSC System Time Table (A65)</doc>
      </member>
      <member name="atsc_rrt" value="17" c:identifier="GST_MPEGTS_SECTION_ATSC_RRT">
      </member>
      <member name="scte_sit" value="18" c:identifier="GST_MPEGTS_SECTION_SCTE_SIT">
        <doc xml:space="preserve">SCTE Splice Information Table (SCTE-35)</doc>
      </member>
    </enumeration>
    <enumeration name="StreamType" c:type="GstMpegtsStreamType">
      <doc xml:space="preserve">Type of mpeg-ts stream type.

These values correspond to the base standard registered types. Depending
on the variant of mpeg-ts being used (Bluray, ATSC, DVB, ...), other
types might also be used, but will not conflict with these.

Corresponds to table 2-34 of ITU H.222.0 | ISO/IEC 13818-1</doc>
      
      <member name="reserved_00" value="0" c:identifier="GST_MPEGTS_STREAM_TYPE_RESERVED_00">
        <doc xml:space="preserve">ITU-T | ISO/IEC Reserved</doc>
      </member>
      <member name="video_mpeg1" value="1" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_MPEG1">
        <doc xml:space="preserve">ISO/IEC 11172-2 Video</doc>
      </member>
      <member name="video_mpeg2" value="2" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_MPEG2">
        <doc xml:space="preserve">Rec. ITU-T H.262 | ISO/IEC 13818-2
Video or ISO/IEC 11172-2 constrained parameter video stream</doc>
      </member>
      <member name="audio_mpeg1" value="3" c:identifier="GST_MPEGTS_STREAM_TYPE_AUDIO_MPEG1">
        <doc xml:space="preserve">ISO/IEC 11172-3 Audio</doc>
      </member>
      <member name="audio_mpeg2" value="4" c:identifier="GST_MPEGTS_STREAM_TYPE_AUDIO_MPEG2">
        <doc xml:space="preserve">ISO/IEC 13818-3 Audio</doc>
      </member>
      <member name="private_sections" value="5" c:identifier="GST_MPEGTS_STREAM_TYPE_PRIVATE_SECTIONS">
        <doc xml:space="preserve">private sections</doc>
      </member>
      <member name="private_pes_packets" value="6" c:identifier="GST_MPEGTS_STREAM_TYPE_PRIVATE_PES_PACKETS">
        <doc xml:space="preserve">PES packets containing private data</doc>
      </member>
      <member name="mheg" value="7" c:identifier="GST_MPEGTS_STREAM_TYPE_MHEG">
        <doc xml:space="preserve">ISO/IEC 13522 MHEG</doc>
      </member>
      <member name="dsm_cc" value="8" c:identifier="GST_MPEGTS_STREAM_TYPE_DSM_CC">
        <doc xml:space="preserve">Annex A DSM-CC</doc>
      </member>
      <member name="h_222_1" value="9" c:identifier="GST_MPEGTS_STREAM_TYPE_H_222_1">
        <doc xml:space="preserve">Rec. ITU-T H.222.1</doc>
      </member>
      <member name="dsmcc_a" value="10" c:identifier="GST_MPEGTS_STREAM_TYPE_DSMCC_A">
        <doc xml:space="preserve">ISO/IEC 13818-6 type A</doc>
      </member>
      <member name="dsmcc_b" value="11" c:identifier="GST_MPEGTS_STREAM_TYPE_DSMCC_B">
        <doc xml:space="preserve">ISO/IEC 13818-6 type B</doc>
      </member>
      <member name="dsmcc_c" value="12" c:identifier="GST_MPEGTS_STREAM_TYPE_DSMCC_C">
        <doc xml:space="preserve">ISO/IEC 13818-6 type C</doc>
      </member>
      <member name="dsmcc_d" value="13" c:identifier="GST_MPEGTS_STREAM_TYPE_DSMCC_D">
        <doc xml:space="preserve">ISO/IEC 13818-6 type D</doc>
      </member>
      <member name="auxiliary" value="14" c:identifier="GST_MPEGTS_STREAM_TYPE_AUXILIARY">
        <doc xml:space="preserve">auxiliary streams</doc>
      </member>
      <member name="audio_aac_adts" value="15" c:identifier="GST_MPEGTS_STREAM_TYPE_AUDIO_AAC_ADTS">
        <doc xml:space="preserve">ISO/IEC 13818-7 Audio with ADTS
transport syntax</doc>
      </member>
      <member name="video_mpeg4" value="16" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_MPEG4">
        <doc xml:space="preserve">ISO/IEC 14496-2 Visual</doc>
      </member>
      <member name="audio_aac_latm" value="17" c:identifier="GST_MPEGTS_STREAM_TYPE_AUDIO_AAC_LATM">
        <doc xml:space="preserve">ISO/IEC 14496-3 Audio with the LATM
transport syntax as defined in ISO/IEC 14496-3</doc>
      </member>
      <member name="sl_flexmux_pes_packets" value="18" c:identifier="GST_MPEGTS_STREAM_TYPE_SL_FLEXMUX_PES_PACKETS">
        <doc xml:space="preserve">ISO/IEC 14496-1
SL-packetized stream or FlexMux stream carried in PES packets</doc>
      </member>
      <member name="sl_flexmux_sections" value="19" c:identifier="GST_MPEGTS_STREAM_TYPE_SL_FLEXMUX_SECTIONS">
        <doc xml:space="preserve">ISO/IEC 14496-1 SL-packetized
stream or FlexMux stream carried in ISO/IEC 14496_sections</doc>
      </member>
      <member name="synchronized_download" value="20" c:identifier="GST_MPEGTS_STREAM_TYPE_SYNCHRONIZED_DOWNLOAD">
        <doc xml:space="preserve">ISO/IEC 13818-6 Synchronized
Download Protocol</doc>
      </member>
      <member name="metadata_pes_packets" value="21" c:identifier="GST_MPEGTS_STREAM_TYPE_METADATA_PES_PACKETS">
        <doc xml:space="preserve">Metadata carried in PES packets</doc>
      </member>
      <member name="metadata_sections" value="22" c:identifier="GST_MPEGTS_STREAM_TYPE_METADATA_SECTIONS">
        <doc xml:space="preserve">Metadata carried in metadata_sections</doc>
      </member>
      <member name="metadata_data_carousel" value="23" c:identifier="GST_MPEGTS_STREAM_TYPE_METADATA_DATA_CAROUSEL">
        <doc xml:space="preserve">Metadata carried in ISO/IEC
13818-6 Data Carousel</doc>
      </member>
      <member name="metadata_object_carousel" value="24" c:identifier="GST_MPEGTS_STREAM_TYPE_METADATA_OBJECT_CAROUSEL">
        <doc xml:space="preserve">Metadata carried in
ISO/IEC 13818-6 Object Carousel</doc>
      </member>
      <member name="metadata_synchronized_download" value="25" c:identifier="GST_MPEGTS_STREAM_TYPE_METADATA_SYNCHRONIZED_DOWNLOAD">
        <doc xml:space="preserve">Metadata carried in
ISO/IEC 13818-6 Synchronized Download Protocol</doc>
      </member>
      <member name="mpeg2_ipmp" value="26" c:identifier="GST_MPEGTS_STREAM_TYPE_MPEG2_IPMP">
        <doc xml:space="preserve">IPMP stream (defined in ISO/IEC 13818-11,
MPEG-2 IPMP)</doc>
      </member>
      <member name="video_h264" value="27" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_H264">
        <doc xml:space="preserve">AVC video stream conforming to one or
more profiles defined in Annex A of Rec. ITU-T H.264 | ISO/IEC 14496-10 or
AVC video sub-bitstream of SVC as defined in 2.1.78 or MVC base view
sub-bitstream, as defined in 2.1.85, or AVC video sub-bitstream of MVC, as
defined in 2.1.88</doc>
      </member>
      <member name="audio_aac_clean" value="28" c:identifier="GST_MPEGTS_STREAM_TYPE_AUDIO_AAC_CLEAN">
        <doc xml:space="preserve">ISO/IEC 14496-3 Audio, without
using any additional transport syntax, such as DST, ALS and SLS</doc>
      </member>
      <member name="mpeg4_timed_text" value="29" c:identifier="GST_MPEGTS_STREAM_TYPE_MPEG4_TIMED_TEXT">
        <doc xml:space="preserve">ISO/IEC 14496-17 Text</doc>
      </member>
      <member name="video_rvc" value="30" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_RVC">
        <doc xml:space="preserve">Auxiliary video stream as defined in
ISO/IEC 23002-3</doc>
      </member>
      <member name="video_h264_svc_sub_bitstream" value="31" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_H264_SVC_SUB_BITSTREAM">
        <doc xml:space="preserve">SVC video sub-bitstream
of an AVC video stream conforming to one or more profiles defined in Annex G
of Rec. ITU-T H.264 | ISO/IEC 14496-10</doc>
      </member>
      <member name="video_h264_mvc_sub_bitstream" value="32" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_H264_MVC_SUB_BITSTREAM">
        <doc xml:space="preserve">MVC video sub-bitstream
of an AVC video stream conforming to one or more profiles defined in Annex H
of Rec. ITU-T H.264 | ISO/IEC 14496-10</doc>
      </member>
      <member name="video_jp2k" value="33" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_JP2K">
        <doc xml:space="preserve">Video stream conforming to one or more
profiles as defined in Rec. ITU-T T.800 | ISO/IEC 15444-1</doc>
      </member>
      <member name="video_mpeg2_stereo_additional_view" value="34" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_MPEG2_STEREO_ADDITIONAL_VIEW">
        <doc xml:space="preserve">Additional view
Rec. ITU-T H.262 | ISO/IEC 13818-2 video stream for service-compatible
stereoscopic 3D services</doc>
      </member>
      <member name="video_h264_stereo_additional_view" value="35" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_H264_STEREO_ADDITIONAL_VIEW">
        <doc xml:space="preserve">Additional view
Rec. ITU-T H.264 | ISO/IEC 14496-10 video stream conforming to one or more
profiles defined in Annex A for service-compatible stereoscopic 3D services</doc>
      </member>
      <member name="video_hevc" value="36" c:identifier="GST_MPEGTS_STREAM_TYPE_VIDEO_HEVC">
      </member>
      <member name="ipmp_stream" value="127" c:identifier="GST_MPEGTS_STREAM_TYPE_IPMP_STREAM">
        <doc xml:space="preserve">IPMP stream</doc>
      </member>
    </enumeration>
    <record name="T2DeliverySystemCell" c:type="GstMpegtsT2DeliverySystemCell" glib:type-name="GstMpegtsT2DeliverySystemCell" glib:get-type="gst_mpegts_t2_delivery_system_cell_get_type" c:symbol-prefix="t2_delivery_system_cell">
      
      <field name="cell_id" writable="1">
        <doc xml:space="preserve">id of the cell</doc>
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="centre_frequencies" writable="1">
        <doc xml:space="preserve">centre frequencies in Hz</doc>
        <array name="GLib.Array" c:type="GArray*">
          <type name="guint32"/>
        </array>
      </field>
      <field name="sub_cells" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="T2DeliverySystemCellExtension"/>
        </array>
      </field>
    </record>
    <record name="T2DeliverySystemCellExtension" c:type="GstMpegtsT2DeliverySystemCellExtension" glib:type-name="GstMpegtsT2DeliverySystemCellExtension" glib:get-type="gst_mpegts_t2_delivery_system_cell_extension_get_type" c:symbol-prefix="t2_delivery_system_cell_extension">
      
      <field name="cell_id_extension" writable="1">
        <doc xml:space="preserve">id of the sub cell</doc>
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="transposer_frequency" writable="1">
        <doc xml:space="preserve">centre frequency of the sub cell in Hz</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
    </record>
    <record name="T2DeliverySystemDescriptor" c:type="GstMpegtsT2DeliverySystemDescriptor" glib:type-name="GstMpegtsT2DeliverySystemDescriptor" glib:get-type="gst_mpegts_t2_delivery_system_descriptor_get_type" c:symbol-prefix="t2_delivery_system_descriptor">
      <doc xml:space="preserve">describe DVB-T2 transmissions according to EN 302 755</doc>
      
      <field name="plp_id" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="t2_system_id" writable="1">
        <type name="guint16" c:type="guint16"/>
      </field>
      <field name="siso_miso" writable="1">
        <type name="guint8" c:type="guint8"/>
      </field>
      <field name="bandwidth" writable="1">
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="guard_interval" writable="1">
        <type name="TerrestrialGuardInterval" c:type="GstMpegtsTerrestrialGuardInterval"/>
      </field>
      <field name="transmission_mode" writable="1">
        <type name="TerrestrialTransmissionMode" c:type="GstMpegtsTerrestrialTransmissionMode"/>
      </field>
      <field name="other_frequency" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="tfs" writable="1">
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="cells" writable="1">
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="T2DeliverySystemCell"/>
        </array>
      </field>
      <method name="free" c:identifier="gst_mpegts_t2_delivery_system_descriptor_free">
        
        <return-value transfer-ownership="none">
          <type name="none" c:type="void"/>
        </return-value>
        <parameters>
          <instance-parameter name="source" transfer-ownership="none">
            <type name="T2DeliverySystemDescriptor" c:type="GstMpegtsT2DeliverySystemDescriptor*"/>
          </instance-parameter>
        </parameters>
      </method>
    </record>
    <record name="TOT" c:type="GstMpegtsTOT" glib:type-name="GstMpegtsTOT" glib:get-type="gst_mpegts_tot_get_type" c:symbol-prefix="tot">
      <doc xml:space="preserve">Time Offset Table (EN 300 468)</doc>
      
      <field name="utc_time" writable="1">
        <type name="Gst.DateTime" c:type="GstDateTime*"/>
      </field>
      <field name="descriptors" writable="1">
        <doc xml:space="preserve">List of descriptors</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </field>
    </record>
    <record name="TerrestrialDeliverySystemDescriptor" c:type="GstMpegtsTerrestrialDeliverySystemDescriptor" glib:type-name="GstMpegtsTerrestrialDeliverySystemDescriptor" glib:get-type="gst_mpegts_terrestrial_delivery_system_descriptor_get_type" c:symbol-prefix="terrestrial_delivery_system_descriptor">
      <doc xml:space="preserve">Terrestrial Delivery System Descriptor (EN 300 468 v.1.13.1)</doc>
      
      <field name="frequency" writable="1">
        <doc xml:space="preserve">the frequency in Hz (Hertz)</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="bandwidth" writable="1">
        <doc xml:space="preserve">the bandwidth in Hz (Hertz)</doc>
        <type name="guint32" c:type="guint32"/>
      </field>
      <field name="priority" writable="1">
        <doc xml:space="preserve">%TRUE High Priority %FALSE Low Priority</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="time_slicing" writable="1">
        <doc xml:space="preserve">%TRUE no time slicing %FALSE time slicing</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="mpe_fec" writable="1">
        <doc xml:space="preserve">%TRUE no mpe-fec is used %FALSE mpe-fec is use</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
      <field name="constellation" writable="1">
        <doc xml:space="preserve">the constellation</doc>
        <type name="ModulationType" c:type="GstMpegtsModulationType"/>
      </field>
      <field name="hierarchy" writable="1">
        <doc xml:space="preserve">the hierarchy</doc>
        <type name="TerrestrialHierarchy" c:type="GstMpegtsTerrestrialHierarchy"/>
      </field>
      <field name="code_rate_hp" writable="1">
        <type name="DVBCodeRate" c:type="GstMpegtsDVBCodeRate"/>
      </field>
      <field name="code_rate_lp" writable="1">
        <type name="DVBCodeRate" c:type="GstMpegtsDVBCodeRate"/>
      </field>
      <field name="guard_interval" writable="1">
        <type name="TerrestrialGuardInterval" c:type="GstMpegtsTerrestrialGuardInterval"/>
      </field>
      <field name="transmission_mode" writable="1">
        <type name="TerrestrialTransmissionMode" c:type="GstMpegtsTerrestrialTransmissionMode"/>
      </field>
      <field name="other_frequency" writable="1">
        <doc xml:space="preserve">%TRUE more frequency are use, else not</doc>
        <type name="gboolean" c:type="gboolean"/>
      </field>
    </record>
    <enumeration name="TerrestrialGuardInterval" c:type="GstMpegtsTerrestrialGuardInterval">
      
      <member name="1_32" value="0" c:identifier="GST_MPEGTS_GUARD_INTERVAL_1_32">
      </member>
      <member name="1_16" value="1" c:identifier="GST_MPEGTS_GUARD_INTERVAL_1_16">
      </member>
      <member name="1_8" value="2" c:identifier="GST_MPEGTS_GUARD_INTERVAL_1_8">
      </member>
      <member name="1_4" value="3" c:identifier="GST_MPEGTS_GUARD_INTERVAL_1_4">
      </member>
      <member name="auto" value="4" c:identifier="GST_MPEGTS_GUARD_INTERVAL_AUTO">
      </member>
      <member name="1_128" value="5" c:identifier="GST_MPEGTS_GUARD_INTERVAL_1_128">
      </member>
      <member name="19_128" value="6" c:identifier="GST_MPEGTS_GUARD_INTERVAL_19_128">
      </member>
      <member name="19_256" value="7" c:identifier="GST_MPEGTS_GUARD_INTERVAL_19_256">
      </member>
      <member name="pn420" value="8" c:identifier="GST_MPEGTS_GUARD_INTERVAL_PN420">
      </member>
      <member name="pn595" value="9" c:identifier="GST_MPEGTS_GUARD_INTERVAL_PN595">
      </member>
      <member name="pn945" value="10" c:identifier="GST_MPEGTS_GUARD_INTERVAL_PN945">
      </member>
    </enumeration>
    <enumeration name="TerrestrialHierarchy" c:type="GstMpegtsTerrestrialHierarchy">
      
      <member name="none" value="0" c:identifier="GST_MPEGTS_HIERARCHY_NONE">
      </member>
      <member name="1" value="1" c:identifier="GST_MPEGTS_HIERARCHY_1">
      </member>
      <member name="2" value="2" c:identifier="GST_MPEGTS_HIERARCHY_2">
      </member>
      <member name="4" value="3" c:identifier="GST_MPEGTS_HIERARCHY_4">
      </member>
      <member name="auto" value="4" c:identifier="GST_MPEGTS_HIERARCHY_AUTO">
      </member>
    </enumeration>
    <enumeration name="TerrestrialTransmissionMode" c:type="GstMpegtsTerrestrialTransmissionMode">
      
      <member name="2k" value="0" c:identifier="GST_MPEGTS_TRANSMISSION_MODE_2K">
      </member>
      <member name="8k" value="1" c:identifier="GST_MPEGTS_TRANSMISSION_MODE_8K">
      </member>
      <member name="auto" value="2" c:identifier="GST_MPEGTS_TRANSMISSION_MODE_AUTO">
      </member>
      <member name="4k" value="3" c:identifier="GST_MPEGTS_TRANSMISSION_MODE_4K">
      </member>
      <member name="1k" value="4" c:identifier="GST_MPEGTS_TRANSMISSION_MODE_1K">
      </member>
      <member name="16k" value="5" c:identifier="GST_MPEGTS_TRANSMISSION_MODE_16K">
      </member>
      <member name="32k" value="6" c:identifier="GST_MPEGTS_TRANSMISSION_MODE_32K">
      </member>
      <member name="c1" value="7" c:identifier="GST_MPEGTS_TRANSMISSION_MODE_C1">
      </member>
      <member name="c3780" value="8" c:identifier="GST_MPEGTS_TRANSMISSION_MODE_C3780">
      </member>
    </enumeration>
    <function name="descriptor_from_custom" c:identifier="gst_mpegts_descriptor_from_custom" moved-to="Descriptor.from_custom">
      <doc xml:space="preserve">Creates a #GstMpegtsDescriptor with custom @tag and @data</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">#GstMpegtsDescriptor</doc>
        <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
      </return-value>
      <parameters>
        <parameter name="tag" transfer-ownership="none">
          <doc xml:space="preserve">descriptor tag</doc>
          <type name="guint8" c:type="guint8"/>
        </parameter>
        <parameter name="data" transfer-ownership="none">
          <doc xml:space="preserve">descriptor data (after tag and length field)</doc>
          <array length="2" zero-terminated="0" c:type="const guint8*">
            <type name="guint8" c:type="guint8"/>
          </array>
        </parameter>
        <parameter name="length" transfer-ownership="none">
          <doc xml:space="preserve">length of @data</doc>
          <type name="gsize" c:type="gsize"/>
        </parameter>
      </parameters>
    </function>
    <function name="descriptor_from_custom_with_extension" c:identifier="gst_mpegts_descriptor_from_custom_with_extension" moved-to="Descriptor.from_custom_with_extension">
      <doc xml:space="preserve">Creates a #GstMpegtsDescriptor with custom @tag, @tag_extension and @data</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">#GstMpegtsDescriptor</doc>
        <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
      </return-value>
      <parameters>
        <parameter name="tag" transfer-ownership="none">
          <doc xml:space="preserve">descriptor tag</doc>
          <type name="guint8" c:type="guint8"/>
        </parameter>
        <parameter name="tag_extension" transfer-ownership="none">
          <doc xml:space="preserve">descriptor tag extension</doc>
          <type name="guint8" c:type="guint8"/>
        </parameter>
        <parameter name="data" transfer-ownership="none">
          <doc xml:space="preserve">descriptor data (after tag and length field)</doc>
          <array length="3" zero-terminated="0" c:type="const guint8*">
            <type name="guint8" c:type="guint8"/>
          </array>
        </parameter>
        <parameter name="length" transfer-ownership="none">
          <doc xml:space="preserve">length of @data</doc>
          <type name="gsize" c:type="gsize"/>
        </parameter>
      </parameters>
    </function>
    <function name="descriptor_from_dvb_network_name" c:identifier="gst_mpegts_descriptor_from_dvb_network_name" moved-to="Descriptor.from_dvb_network_name">
      <doc xml:space="preserve">Creates a #GstMpegtsDescriptor to be a %GST_MTS_DESC_DVB_NETWORK_NAME,
with the network name @name. The data field of the #GstMpegtsDescriptor
will be allocated, and transferred to the caller.</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">the #GstMpegtsDescriptor or %NULL on fail</doc>
        <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
      </return-value>
      <parameters>
        <parameter name="name" transfer-ownership="none">
          <doc xml:space="preserve">the network name to set</doc>
          <type name="utf8" c:type="const gchar*"/>
        </parameter>
      </parameters>
    </function>
    <function name="descriptor_from_dvb_service" c:identifier="gst_mpegts_descriptor_from_dvb_service" moved-to="Descriptor.from_dvb_service">
      <doc xml:space="preserve">Fills a #GstMpegtsDescriptor to be a %GST_MTS_DESC_DVB_SERVICE.
The data field of the #GstMpegtsDescriptor will be allocated,
and transferred to the caller.</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">the #GstMpegtsDescriptor or %NULL on fail</doc>
        <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
      </return-value>
      <parameters>
        <parameter name="service_type" transfer-ownership="none">
          <doc xml:space="preserve">Service type defined as a #GstMpegtsDVBServiceType</doc>
          <type name="DVBServiceType" c:type="GstMpegtsDVBServiceType"/>
        </parameter>
        <parameter name="service_name" transfer-ownership="none" nullable="1" allow-none="1">
          <doc xml:space="preserve">Name of the service</doc>
          <type name="utf8" c:type="const gchar*"/>
        </parameter>
        <parameter name="service_provider" transfer-ownership="none" nullable="1" allow-none="1">
          <doc xml:space="preserve">Name of the service provider</doc>
          <type name="utf8" c:type="const gchar*"/>
        </parameter>
      </parameters>
    </function>
    <function name="descriptor_from_dvb_subtitling" c:identifier="gst_mpegts_descriptor_from_dvb_subtitling" moved-to="Descriptor.from_dvb_subtitling">
      
      <return-value transfer-ownership="full">
        <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
      </return-value>
      <parameters>
        <parameter name="lang" transfer-ownership="none">
          <doc xml:space="preserve">a string containing the ISO639 language</doc>
          <type name="utf8" c:type="const gchar*"/>
        </parameter>
        <parameter name="type" transfer-ownership="none">
          <doc xml:space="preserve">subtitling type</doc>
          <type name="guint8" c:type="guint8"/>
        </parameter>
        <parameter name="composition" transfer-ownership="none">
          <doc xml:space="preserve">composition page id</doc>
          <type name="guint16" c:type="guint16"/>
        </parameter>
        <parameter name="ancillary" transfer-ownership="none">
          <doc xml:space="preserve">ancillary page id</doc>
          <type name="guint16" c:type="guint16"/>
        </parameter>
      </parameters>
    </function>
    <function name="descriptor_from_iso_639_language" c:identifier="gst_mpegts_descriptor_from_iso_639_language" moved-to="Descriptor.from_iso_639_language">
      <doc xml:space="preserve">Creates a %GST_MTS_DESC_ISO_639_LANGUAGE #GstMpegtsDescriptor with
a single language</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">#GstMpegtsDescriptor, %NULL on failure</doc>
        <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
      </return-value>
      <parameters>
        <parameter name="language" transfer-ownership="none">
          <doc xml:space="preserve">ISO-639-2 language 3-char code</doc>
          <type name="utf8" c:type="const gchar*"/>
        </parameter>
      </parameters>
    </function>
    <function name="descriptor_from_registration" c:identifier="gst_mpegts_descriptor_from_registration" moved-to="Descriptor.from_registration">
      <doc xml:space="preserve">Creates a %GST_MTS_DESC_REGISTRATION #GstMpegtsDescriptor</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">#GstMpegtsDescriptor, %NULL on failure</doc>
        <type name="Descriptor" c:type="GstMpegtsDescriptor*"/>
      </return-value>
      <parameters>
        <parameter name="format_identifier" transfer-ownership="none">
          <doc xml:space="preserve">a 4 character format identifier string</doc>
          <type name="utf8" c:type="const gchar*"/>
        </parameter>
        <parameter name="additional_info" transfer-ownership="none" nullable="1" allow-none="1">
          <doc xml:space="preserve">pointer to optional additional info</doc>
          <array length="2" zero-terminated="0" c:type="guint8*">
            <type name="guint8" c:type="guint8"/>
          </array>
        </parameter>
        <parameter name="additional_info_length" transfer-ownership="none">
          <doc xml:space="preserve">length of the optional @additional_info</doc>
          <type name="gsize" c:type="gsize"/>
        </parameter>
      </parameters>
    </function>
    <function name="dvb_component_descriptor_free" c:identifier="gst_mpegts_dvb_component_descriptor_free">
      
      <return-value transfer-ownership="none">
        <type name="none" c:type="void"/>
      </return-value>
      <parameters>
        <parameter name="source" transfer-ownership="none">
          <type name="ComponentDescriptor" c:type="GstMpegtsComponentDescriptor*"/>
        </parameter>
      </parameters>
    </function>
    <function name="event_parse_mpegts_section" c:identifier="gst_event_parse_mpegts_section">
      <doc xml:space="preserve">Extracts the #GstMpegtsSection contained in the @event #GstEvent</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">The extracted #GstMpegtsSection</doc>
        <type name="Section" c:type="GstMpegtsSection*"/>
      </return-value>
      <parameters>
        <parameter name="event" transfer-ownership="none">
          <doc xml:space="preserve">#GstEvent containing a #GstMpegtsSection</doc>
          <type name="Gst.Event" c:type="GstEvent*"/>
        </parameter>
      </parameters>
    </function>
    <function name="find_descriptor" c:identifier="gst_mpegts_find_descriptor">
      <doc xml:space="preserve">Finds the first descriptor of type @tag in the array.

Note: To look for descriptors that can be present more than once in an
array of descriptors, iterate the #GArray manually.</doc>
      
      <return-value transfer-ownership="none">
        <doc xml:space="preserve">the first descriptor matching @tag, else %NULL.</doc>
        <type name="Descriptor" c:type="const GstMpegtsDescriptor*"/>
      </return-value>
      <parameters>
        <parameter name="descriptors" transfer-ownership="none">
          <doc xml:space="preserve">an array
of #GstMpegtsDescriptor</doc>
          <array name="GLib.PtrArray" c:type="GPtrArray*">
            <type name="Descriptor"/>
          </array>
        </parameter>
        <parameter name="tag" transfer-ownership="none">
          <doc xml:space="preserve">the tag to look for</doc>
          <type name="guint8" c:type="guint8"/>
        </parameter>
      </parameters>
    </function>
    <function name="initialize" c:identifier="gst_mpegts_initialize">
      <doc xml:space="preserve">Initializes the MPEG-TS helper library. Must be called before any
usage.</doc>
      
      <return-value transfer-ownership="none">
        <type name="none" c:type="void"/>
      </return-value>
    </function>
    <function name="message_new_mpegts_section" c:identifier="gst_message_new_mpegts_section">
      <doc xml:space="preserve">Creates a new #GstMessage for a @GstMpegtsSection.</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">The new #GstMessage to be posted, or %NULL if the
section is not valid.</doc>
        <type name="Gst.Message" c:type="GstMessage*"/>
      </return-value>
      <parameters>
        <parameter name="parent" transfer-ownership="none">
          <doc xml:space="preserve">The creator of the message</doc>
          <type name="Gst.Object" c:type="GstObject*"/>
        </parameter>
        <parameter name="section" transfer-ownership="none">
          <doc xml:space="preserve">The #GstMpegtsSection to put in a message</doc>
          <type name="Section" c:type="GstMpegtsSection*"/>
        </parameter>
      </parameters>
    </function>
    <function name="message_parse_mpegts_section" c:identifier="gst_message_parse_mpegts_section">
      <doc xml:space="preserve">Returns the #GstMpegtsSection contained in a message.</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">the contained #GstMpegtsSection, or %NULL.</doc>
        <type name="Section" c:type="GstMpegtsSection*"/>
      </return-value>
      <parameters>
        <parameter name="message" transfer-ownership="none">
          <doc xml:space="preserve">a #GstMessage</doc>
          <type name="Gst.Message" c:type="GstMessage*"/>
        </parameter>
      </parameters>
    </function>
    <function name="parse_descriptors" c:identifier="gst_mpegts_parse_descriptors">
      <doc xml:space="preserve">Parses the descriptors present in @buffer and returns them as an
array.

Note: The data provided in @buffer will not be copied.</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">an
array of the parsed descriptors or %NULL if there was an error.
Release with #g_array_unref when done with it.</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="Descriptor"/>
        </array>
      </return-value>
      <parameters>
        <parameter name="buffer" transfer-ownership="none">
          <doc xml:space="preserve">descriptors to parse</doc>
          <type name="guint8" c:type="guint8*"/>
        </parameter>
        <parameter name="buf_len" transfer-ownership="none">
          <doc xml:space="preserve">Size of @buffer</doc>
          <type name="gsize" c:type="gsize"/>
        </parameter>
      </parameters>
    </function>
    <function name="pat_new" c:identifier="gst_mpegts_pat_new">
      <doc xml:space="preserve">Allocates a new #GPtrArray for #GstMpegtsPatProgram</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">A newly allocated #GPtrArray</doc>
        <array name="GLib.PtrArray" c:type="GPtrArray*">
          <type name="PatProgram"/>
        </array>
      </return-value>
    </function>
    <function name="scte_cancel_new" c:identifier="gst_mpegts_scte_cancel_new">
      <doc xml:space="preserve">Allocates and initializes a new INSERT command #GstMpegtsSCTESIT
setup to cancel the specified @event_id.</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">A newly allocated #GstMpegtsSCTESIT</doc>
        <type name="SCTESIT" c:type="GstMpegtsSCTESIT*"/>
      </return-value>
      <parameters>
        <parameter name="event_id" transfer-ownership="none">
          <doc xml:space="preserve">The event ID to cancel.</doc>
          <type name="guint32" c:type="guint32"/>
        </parameter>
      </parameters>
    </function>
    <function name="scte_null_new" c:identifier="gst_mpegts_scte_null_new">
      <doc xml:space="preserve">Allocates and initializes a NULL command #GstMpegtsSCTESIT.</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">A newly allocated #GstMpegtsSCTESIT</doc>
        <type name="SCTESIT" c:type="GstMpegtsSCTESIT*"/>
      </return-value>
    </function>
    <function name="scte_splice_in_new" c:identifier="gst_mpegts_scte_splice_in_new">
      <doc xml:space="preserve">Allocates and initializes a new "Splice In" INSERT command
#GstMpegtsSCTESIT for the given @event_id and @splice_time.

If the @splice_time is #G_MAXUINT64 then the event will be
immediate as opposed to for the target @splice_time.</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">A newly allocated #GstMpegtsSCTESIT</doc>
        <type name="SCTESIT" c:type="GstMpegtsSCTESIT*"/>
      </return-value>
      <parameters>
        <parameter name="event_id" transfer-ownership="none">
          <doc xml:space="preserve">The event ID.</doc>
          <type name="guint32" c:type="guint32"/>
        </parameter>
        <parameter name="splice_time" transfer-ownership="none">
          <doc xml:space="preserve">The PCR time for the splice event</doc>
          <type name="guint64" c:type="guint64"/>
        </parameter>
      </parameters>
    </function>
    <function name="scte_splice_out_new" c:identifier="gst_mpegts_scte_splice_out_new">
      <doc xml:space="preserve">Allocates and initializes a new "Splice Out" INSERT command
#GstMpegtsSCTESIT for the given @event_id, @splice_time and
duration.

If the @splice_time is #G_MAXUINT64 then the event will be
immediate as opposed to for the target @splice_time.

If the @duration is 0 it won't be specified in the event.</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">A newly allocated #GstMpegtsSCTESIT</doc>
        <type name="SCTESIT" c:type="GstMpegtsSCTESIT*"/>
      </return-value>
      <parameters>
        <parameter name="event_id" transfer-ownership="none">
          <doc xml:space="preserve">The event ID.</doc>
          <type name="guint32" c:type="guint32"/>
        </parameter>
        <parameter name="splice_time" transfer-ownership="none">
          <doc xml:space="preserve">The PCR time for the splice event</doc>
          <type name="guint64" c:type="guint64"/>
        </parameter>
        <parameter name="duration" transfer-ownership="none">
          <doc xml:space="preserve">The optional duration.</doc>
          <type name="guint64" c:type="guint64"/>
        </parameter>
      </parameters>
    </function>
    <function name="section_from_atsc_mgt" c:identifier="gst_mpegts_section_from_atsc_mgt" moved-to="Section.from_atsc_mgt" version="1.18">
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">the #GstMpegtsSection</doc>
        <type name="Section" c:type="GstMpegtsSection*"/>
      </return-value>
      <parameters>
        <parameter name="mgt" transfer-ownership="full">
          <doc xml:space="preserve">a #GstMpegtsAtscMGT to create the #GstMpegtsSection from</doc>
          <type name="AtscMGT" c:type="GstMpegtsAtscMGT*"/>
        </parameter>
      </parameters>
    </function>
    <function name="section_from_atsc_rrt" c:identifier="gst_mpegts_section_from_atsc_rrt" moved-to="Section.from_atsc_rrt">
      
      <return-value transfer-ownership="full">
        <type name="Section" c:type="GstMpegtsSection*"/>
      </return-value>
      <parameters>
        <parameter name="rrt" transfer-ownership="none">
          <type name="AtscRRT" c:type="GstMpegtsAtscRRT*"/>
        </parameter>
      </parameters>
    </function>
    <function name="section_from_atsc_stt" c:identifier="gst_mpegts_section_from_atsc_stt" moved-to="Section.from_atsc_stt">
      
      <return-value transfer-ownership="full">
        <type name="Section" c:type="GstMpegtsSection*"/>
      </return-value>
      <parameters>
        <parameter name="stt" transfer-ownership="none">
          <type name="AtscSTT" c:type="GstMpegtsAtscSTT*"/>
        </parameter>
      </parameters>
    </function>
    <function name="section_from_nit" c:identifier="gst_mpegts_section_from_nit" moved-to="Section.from_nit">
      <doc xml:space="preserve">Ownership of @nit is taken. The data in @nit is managed by the #GstMpegtsSection</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">the #GstMpegtsSection</doc>
        <type name="Section" c:type="GstMpegtsSection*"/>
      </return-value>
      <parameters>
        <parameter name="nit" transfer-ownership="full">
          <doc xml:space="preserve">a #GstMpegtsNIT to create the #GstMpegtsSection from</doc>
          <type name="NIT" c:type="GstMpegtsNIT*"/>
        </parameter>
      </parameters>
    </function>
    <function name="section_from_pat" c:identifier="gst_mpegts_section_from_pat" moved-to="Section.from_pat">
      <doc xml:space="preserve">Creates a PAT #GstMpegtsSection from the @programs array of #GstMpegtsPatPrograms</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">a #GstMpegtsSection</doc>
        <type name="Section" c:type="GstMpegtsSection*"/>
      </return-value>
      <parameters>
        <parameter name="programs" transfer-ownership="full">
          <doc xml:space="preserve">an array of #GstMpegtsPatProgram</doc>
          <array name="GLib.PtrArray" c:type="GPtrArray*">
            <type name="PatProgram"/>
          </array>
        </parameter>
        <parameter name="ts_id" transfer-ownership="none">
          <doc xml:space="preserve">Transport stream ID of the PAT</doc>
          <type name="guint16" c:type="guint16"/>
        </parameter>
      </parameters>
    </function>
    <function name="section_from_pmt" c:identifier="gst_mpegts_section_from_pmt" moved-to="Section.from_pmt">
      <doc xml:space="preserve">Creates a #GstMpegtsSection from @pmt that is bound to @pid</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">#GstMpegtsSection</doc>
        <type name="Section" c:type="GstMpegtsSection*"/>
      </return-value>
      <parameters>
        <parameter name="pmt" transfer-ownership="full">
          <doc xml:space="preserve">a #GstMpegtsPMT to create a #GstMpegtsSection from</doc>
          <type name="PMT" c:type="GstMpegtsPMT*"/>
        </parameter>
        <parameter name="pid" transfer-ownership="none">
          <doc xml:space="preserve">The PID that the #GstMpegtsPMT belongs to</doc>
          <type name="guint16" c:type="guint16"/>
        </parameter>
      </parameters>
    </function>
    <function name="section_from_scte_sit" c:identifier="gst_mpegts_section_from_scte_sit" moved-to="Section.from_scte_sit">
      <doc xml:space="preserve">Ownership of @sit is taken. The data in @sit is managed by the #GstMpegtsSection</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">the #GstMpegtsSection</doc>
        <type name="Section" c:type="GstMpegtsSection*"/>
      </return-value>
      <parameters>
        <parameter name="sit" transfer-ownership="full">
          <doc xml:space="preserve">a #GstMpegtsSCTESIT to create the #GstMpegtsSection from</doc>
          <type name="SCTESIT" c:type="GstMpegtsSCTESIT*"/>
        </parameter>
        <parameter name="pid" transfer-ownership="none">
          <type name="guint16" c:type="guint16"/>
        </parameter>
      </parameters>
    </function>
    <function name="section_from_sdt" c:identifier="gst_mpegts_section_from_sdt" moved-to="Section.from_sdt">
      <doc xml:space="preserve">Ownership of @sdt is taken. The data in @sdt is managed by the #GstMpegtsSection</doc>
      
      <return-value transfer-ownership="full">
        <doc xml:space="preserve">the #GstMpegtsSection</doc>
        <type name="Section" c:type="GstMpegtsSection*"/>
      </return-value>
      <parameters>
        <parameter name="sdt" transfer-ownership="full">
          <doc xml:space="preserve">a #GstMpegtsSDT to create the #GstMpegtsSection from</doc>
          <type name="SDT" c:type="GstMpegtsSDT*"/>
        </parameter>
      </parameters>
    </function>
    <function-macro name="section_ref" c:identifier="gst_mpegts_section_ref" introspectable="0">
      
      <parameters>
        <parameter name="section">
        </parameter>
      </parameters>
    </function-macro>
    <function-macro name="section_unref" c:identifier="gst_mpegts_section_unref" introspectable="0">
      
      <parameters>
        <parameter name="section">
        </parameter>
      </parameters>
    </function-macro>
  </namespace>
</repository>
